
##
## Kernel-specific run tool configuration
##

RUN_OPT = --include boot_dir/hw --include image/muen

#
# Muen hardware configuration
#
# The specified file must be relative to the Muen policy directory or an
# absolute path.
#
RUN_OPT += --image-muen-hardware hardware/lenovo-t430s.xml

#
# Muen platform configuration
#
# The specified file must be relative to the Muen policy directory or an
# absolute path.
#
RUN_OPT += --image-muen-platform platform/lenovo-t430s.xml

#
# Directory, where the GNAT toolchain is installed
#
RUN_OPT += --image-muen-gnat-path /opt/gnat

#
# Directory, where the SPARK toolchain is installed
#
RUN_OPT += --image-muen-spark-path /opt/spark

#
# Muen system policy
#
# The specified file must be relative to the Muen policy directory or an
# absolute path.
#
RUN_OPT += --image-muen-system xml/genode-base_hw.xml

#
# Muen system components
#
# Available components are located in the Muen project directory 'components/'.
#
RUN_OPT += --image-muen-components 'libdebuglog libmutime libxhcidbg dbgserver sm time'

#
# External Muen build
#
# Specifies if the Muen kernel should be built automatically.
# If the Muen system is built and integrated externally, i.e. outside
# of the Genode build system, set this parameter to 1.
#
RUN_OPT += --image-muen-external-build 0

