#
# Build
#

if {[have_spec odroid_xu] || [have_spec wand_quad] || [have_spec zynq] || [have_spec imx53] && [have_spec foc]} {
	puts "\n Run script is not supported on this platform. \n";
	exit 0
}

if {[get_cmd_switch --autopilot] && [have_spec linux]} {
	puts "\nAutopilot run is not supported on this platform\n"
	exit 0
}

set build_components { core init test/fb_bench drivers/framebuffer drivers/timer }

source ${genode_dir}/repos/base/run/platform_drv.inc
append_platform_drv_build_components

lappend_if [have_spec gpio] build_components drivers/gpio

build $build_components

create_boot_directory

#
# Generate config
#

proc gpio_drv { } { if {[have_spec rpi] && [have_spec hw]}  { return hw_gpio_drv }
                    if {[have_spec rpi] && [have_spec foc]} { return foc_gpio_drv }
                    return gpio_drv }

append config {
<config>
	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<default caps="100"/>

	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Timer"/></provides>
	</start>}

append_if [have_spec gpio] config "
	<start name=\"[gpio_drv]\" caps=\"140\">
		<resource name=\"RAM\" quantum=\"4M\"/>
		<provides><service name=\"Gpio\"/></provides>
		<config/>
	</start>"

append_if [have_spec sdl] config {
	<start name="fb_sdl">
		<resource name="RAM" quantum="4M"/>
		<provides>
			<service name="Input"/>
			<service name="Framebuffer"/>
		</provides>
	</start>}

append_platform_drv_config

append_if [have_spec framebuffer] config {
	<start name="fb_drv" caps="150">
		<resource name="RAM" quantum="20M"/>
		<provides><service name="Framebuffer"/></provides>
	</start>}

append config {
	<start name="test-fb_bench">
		<!--
		  - We need this big amount of RAM because the VESA driver reports a
		  - large buffer on some hardware and the test mirrors this buffer in
		  - RAM.
		  -->
		<resource name="RAM" quantum="72M"/>
	</start>
</config>}

install_config $config

#
# Boot modules
#

set boot_modules { core ld.lib.so init timer test-fb_bench }

append_platform_drv_boot_modules

lappend_if [have_spec sdl]         boot_modules fb_sdl
lappend_if [have_spec framebuffer] boot_modules fb_drv
lappend_if [have_spec gpio]        boot_modules [gpio_drv]

build_boot_image $boot_modules

# disable QEMU graphic to enable testing on our machines without SDL and X
append qemu_args "-nographic "

run_genode_until {.*--- Framebuffer benchmark finished ---.*\n} 40
