#
# Build
#

set build_components {
	core init
	drivers/timer drivers/wifi
	drivers/rtc
	server/report_rom
	server/ram_fs
	server/fs_rom
	test/lwip/http_srv
	lib/vfs/jitterentropy
}

lappend_if [have_spec gpio]             build_components drivers/gpio

source ${genode_dir}/repos/base/run/platform_drv.inc
append_platform_drv_build_components

build $build_components

create_boot_directory

#
# Generate config
#

set config {
<config verbose="yes">
	<parent-provides>
		<service name="ROM"/>
		<service name="RAM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="CAP"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
		<service name="SIGNAL"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Timer"/> </provides>
	</start>
	<start name="rtc_drv">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Rtc"/> </provides>
	</start>
	<start name="test-lwip_httpsrv">
		<resource name="RAM" quantum="5M"/>
		<config>
			<libc stdout="/dev/log" stderr="/dev/log">
				<vfs> <dir name="dev"> <log/> </dir> </vfs>
			</libc>
		</config>
	</start>
	<start name="report_rom">
		<resource name="RAM" quantum="2M"/>
		<provides> <service name="Report" /> <service name="ROM" /> </provides>
		<config> <rom/> </config>
	</start>
	<start name="config_fs">
		<binary name="ram_fs"/>
		<resource name="RAM" quantum="4M"/>
		<provides> <service name="File_system"/> </provides>
		<config>
			<policy label="config_rom" root="/"/>
			<policy label="wifi_drv -> config" root="/" writeable="yes"/>
			<content>
				<inline name="wlan_configuration">
<selected_network ssid="foobar" protection="WPA-PSK" psk="foobarfoobar"/>
				</inline>
				<inline name="wpa_supplicant.conf"></inline>
			</content>
		</config>
	</start>
	<start name="config_rom">
		<binary name="fs_rom"/>
		<resource name="RAM" quantum="4M"/>
		<provides><service name="ROM"/></provides>
		<route>
			<service name="File_system"> <child name="config_fs" /> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>
	<start name="wifi_drv">
		<resource name="RAM" quantum="32M"/>
		<provides> <service name="Nic"/> </provides>
		<config verbose="yes">
			<libc stdout="/dev/log" stderr="/dev/log" rtc="/dev/rtc">
				<vfs>
					<dir name="dev"> <log/> <rtc/>
						<jitterentropy name="random"/>
						<jitterentropy name="urandom"/>
					</dir>
					<dir name="config"> <fs label="config"/> </dir>
				</vfs>
			</libc>
		</config>
		<route>
			<service name="Rtc"> <any-child /> </service>
			<service name="File_system"> <child name="config_fs"/> </service>
			<service name="Report"> <child name="report_rom"/> </service>
			<service name="ROM"> <if-arg key="label" value="wlan_configuration" /> <child name="config_rom" /> </service>
			<any-service> <parent/> <any-child /> </any-service>
		</route>
	</start>}

append_platform_drv_config

append_if [have_spec gpio] config {
	<start name="gpio_drv">
		<resource name="RAM" quantum="4M"/>
		<provides><service name="Gpio"/></provides>
		<config/>
	</start>}

append config {
</config>
}

install_config $config

set firmware_modules {
	iwlwifi-6000-6.ucode
	iwlwifi-6000g2a-6.ucode
	iwlwifi-6000g2b-6.ucode
	iwlwifi-7260-8.ucode
	iwlwifi-7265-8.ucode
}

#
# Boot modules
#

# generic modules
set boot_modules {
	core init timer rtc_drv ram_fs report_rom fs_rom
	vfs_jitterentropy.lib.so
	ld.lib.so
	libc.lib.so libcrypto.lib.so libssl.lib.so
	wpa_driver_nl80211.lib.so wpa_supplicant.lib.so
	wifi.lib.so
	wifi_drv

	test-lwip_httpsrv lwip.lib.so
}

append boot_modules $firmware_modules

lappend_if [have_spec gpio]             boot_modules gpio_drv

append_platform_drv_boot_modules

build_boot_image $boot_modules

run_genode_until forever

# vi: set ft=tcl :
