#
# \brief  Virtual-machine monitor demo
# \author Stefan Kalkowski
# \date   2015-06-25
#

assert_spec hw_arndale

set build_components {
	core init
	drivers/timer
	drivers/platform
	drivers/uart
	server/vmm
}
build $build_components
create_boot_directory

install_config {
<config verbose="yes">
	<parent-provides>
		<service name="ROM"/>
		<service name="RAM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="CAP"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
		<service name="SIGNAL"/>
		<service name="VM"/>
	</parent-provides>
	<default-route>
		<any-service><parent/><any-child/></any-service>
	</default-route>
	<start name="platform_drv">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Regulator"/></provides>
		<config/>
	</start>
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Timer"/></provides>
	</start>
	<start name="uart_drv">
		<resource name="RAM" quantum="2M"/>
		<provides>
			<service name="Terminal"/>
			<service name="Uart"/>
		</provides>
		<config>
			<policy label="vmm" uart="1"/>
		</config>
	</start>
	<start name="vmm">
		<resource name="RAM" quantum="256M"/>
	</start>
</config>
}


#
# This test uses a Linux kernel built from unmodified vanilla kernel sources
# but using a slightly simplified kernel configuration, as well as device tree
# for a minimal Versatile Express Cortex A15 like emulated board.
#
# The used sources, including the modified device tree and configuration file
# can be found in the following git repository/branch:
#
#   https://github.com/skalk/linux/tree/vexpress-vt
#
# To compile the kernel and device tree blob used in this script, do the
# following steps:
#
# ! git checkout https://github.com/skalk/linux.git
# ! cd linux
# ! git checkout origin/vexpress-vt
# ! make ARCH=arm CROSS_COMPILE=<cross_compiler_prefix> vexpress_config
# ! make ARCH=arm CROSS_COMPILE=<cross_compiler_prefix> -j8 Image
# ! make ARCH=arm CROSS_COMPILE=<cross_compiler_prefix> vexpress-v2p-ca15-tc1.dtb
#

if {![file exists bin/linux]} {
	puts "Download linux kernel ..."
	exec >& /dev/null wget -c -O bin/linux http://genode.org/files/release-15.02/arm_vt/linux
}

if {![file exists bin/dtb]} {
	puts "Download device tree blob ..."
	exec >& /dev/null wget -c -O bin/dtb http://genode.org/files/release-15.02/arm_vt/dtb
}

set boot_modules {
	core init
	platform_drv
	uart_drv
	timer
	vmm
	linux
	dtb
}
build_boot_image $boot_modules

#
# Execute test case
#
run_genode_until {.*\/ #.*} 220
set serial_id [output_spawn_id]
send -i $serial_id "ls\n"
run_genode_until "var" 30 $serial_id
exec rm bin/linux bin/dtb
