#
# \brief  Test for using the lwIP TCP/IP stack over USB
# \author Sebastian Sumpf
# \date   2012-07-06
#
# This test case executes a small HTTP server, it has been used on PandaBoard
# hardware only, though it should execute but not do anything on other hardware
#

#
# Build
#

set build_components {
	core init
	drivers/timer drivers/usb
	test/lwip/http_srv
}

source ${genode_dir}/repos/base/run/platform_drv.inc
append_platform_drv_build_components

lappend_if [have_spec gpio]             build_components drivers/gpio

build $build_components

create_boot_directory

#
# Generate config
#

set config {
<config verbose="yes">
	<parent-provides>
		<service name="ROM"/>
		<service name="RAM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="CAP"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
		<service name="SIGNAL"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Timer"/> </provides>
	</start>
	<start name="usb_drv">
		<resource name="RAM" quantum="12M"/>
		<provides>
			<service name="Nic"/>
		</provides>
		<config uhci="no" ehci="yes" xhci="yes">
			<nic mac="02:00:00:00:01:01" />
		</config>
	</start>
	<start name="test-lwip_httpsrv">
		<resource name="RAM" quantum="2M"/>
		<config>
			<libc stdout="/dev/log">
				<vfs> <dir name="dev"> <log/> </dir> </vfs>
			</libc>
		</config>
	</start>}

append_platform_drv_config

append_if [have_spec gpio] config {
	<start name="gpio_drv">
		<resource name="RAM" quantum="4M"/>
		<provides><service name="Gpio"/></provides>
		<config/>
	</start>}

append config {
</config>
}

install_config $config

#
# Boot modules
#

# generic modules
set boot_modules {
	core init timer
	usb_drv
	ld.lib.so libc.lib.so lwip.lib.so test-lwip_httpsrv
}

append_platform_drv_boot_modules
lappend_if [have_spec gpio]             boot_modules gpio_drv

build_boot_image $boot_modules

append qemu_args " -m 256 -nographic"

run_genode_until forever
# vi: set ft=tcl :
