set use_net 0
set use_ps2 [have_spec ps2]
set use_usb 0
set use_serial 0

set build_components {
	core init virtualbox
	drivers/framebuffer
	drivers/timer
}

source ${genode_dir}/repos/base/run/platform_drv.inc
# override defaults of platform_drv.inc
proc platform_drv_priority {} { return { priority="-1"} }

lappend_if [expr $use_ps2]    build_components drivers/input
lappend_if [expr $use_usb]    build_components drivers/usb
lappend_if [expr $use_serial] build_components server/log_terminal
lappend_if [have_spec x86]    build_components drivers/rtc

lappend_if [expr $use_net]    build_components drivers/nic

append_platform_drv_build_components

build $build_components

create_boot_directory

set config {
<config prio_levels="4">
	<parent-provides>
		<service name="ROM"/>
		<service name="RAM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="CAP"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
		<service name="SIGNAL"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Timer"/></provides>
	</start>}

append_platform_drv_config

append_if [expr $use_ps2] config {
	<start name="ps2_drv" priority="-1">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Input"/></provides>
	</start>}

append_if [expr $use_usb] config {
	<start name="usb_drv" priority="-1">
		<resource name="RAM" quantum="7M"/>
		<provides><service name="Input"/></provides>
		<config uhci="yes" ehci="yes" xhci="yes">
			<hid/>
		</config>
	</start>}

append_if [have_spec framebuffer] config {
	<start name="fb_drv" priority="-1">
		<resource name="RAM" quantum="4M"/>
		<provides><service name="Framebuffer"/></provides>
	</start>}

append_if [have_spec sdl] config {
	<start name="fb_sdl" priority="-1">
		<resource name="RAM" quantum="4M"/>
		<provides>
			<service name="Input"/>
			<service name="Framebuffer"/>
		</provides>
	</start>}

append_if [have_spec x86] config {
	<start name="rtc_drv" priority="-1">
		<resource name="RAM" quantum="1M"/>
		<provides>
			<service name="Rtc"/>
		</provides>
	</start>}

append_if [expr $use_net] config {
	<start name="nic_drv" priority="-1">
		<resource name="RAM" quantum="4M"/>
		<provides><service name="Nic"/></provides>
	</start>
}

append_if [expr $use_serial] config {
	<start name="log_terminal">
		<resource name="RAM" quantum="2M"/>
		<provides>
			<service name="Terminal"/>
		</provides>
	</start>
}

append config {
	<start name="virtualbox" priority="-2">
		<resource name="RAM" quantum="448M"/>
		<config vbox_file="test.vbox" vm_name="TestVM">
			<libc stdout="/dev/log" stderr="/dev/log" rtc="/dev/rtc">
				<vfs>
					<dir name="dev"> <log/> <rtc/> </dir>}

append_if [expr $use_serial] config {
					<dir name="dev"> <terminal/> </dir>}

append config {
					<rom name="test.vbox" />
					<rom name="test.iso" />
				</vfs>
			</libc>
		</config>
	</start>
</config>
}

install_config $config

exec cp ${genode_dir}/repos/ports/run/test.vbox bin/.

set boot_modules { core init timer virtualbox test.iso test.vbox }

# platform-specific modules
lappend_if [expr         $use_usb] boot_modules usb_drv
lappend_if [expr         $use_ps2] boot_modules ps2_drv
lappend_if [have_spec framebuffer] boot_modules fb_drv
lappend_if [have_spec       linux] boot_modules fb_sdl
lappend_if [have_spec         x86] boot_modules rtc_drv

append boot_modules {
	ld.lib.so libc.lib.so libm.lib.so pthread.lib.so libc_lock_pipe.lib.so
	libc_terminal.lib.so libiconv.lib.so stdcxx.lib.so
}

append_if [expr $use_net]          boot_modules { nic_drv }
append_if [expr $use_serial]       boot_modules { log_terminal }

append_platform_drv_boot_modules

build_boot_image $boot_modules

if {[have_include "power_on/qemu"]} {
	append qemu_args " -m 512 "
	append qemu_args " -cpu phenom "
	if {[expr $use_usb]} {
		append qemu_args " -usbdevice mouse -usbdevice keyboard"
	}
}

run_genode_until forever
