#
# Build
#

if {[have_spec hw_odroid_xu]} {
	puts "Run script does not support this platform."
	exit 0
}

set build_components {
	core init
	drivers/timer
	app/decorator
	server/nitpicker server/report_rom
	test/decorator_stress
	drivers/framebuffer drivers/input
}

source ${genode_dir}/repos/base/run/platform_drv.inc
append_platform_drv_build_components

lappend_if [have_spec usb]              build_components drivers/usb
lappend_if [have_spec gpio]             build_components drivers/gpio

build $build_components

create_boot_directory

#
# Generate config
#

append config {
<config>
	<parent-provides>
		<service name="ROM"/>
		<service name="RAM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="CAP"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
		<service name="SIGNAL"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>}

append_if [have_spec sdl] config {
	<start name="fb_sdl">
		<resource name="RAM" quantum="4M"/>
		<provides>
			<service name="Input"/>
			<service name="Framebuffer"/>
		</provides>
	</start>}

append_platform_drv_config

append_if [have_spec framebuffer] config {
	<start name="fb_drv">
		<resource name="RAM" quantum="4M"/>
		<provides><service name="Framebuffer"/></provides>
	</start>}

append_if [have_spec gpio] config {
	<start name="gpio_drv">
		<resource name="RAM" quantum="4M"/>
		<provides><service name="Gpio"/></provides>
		<config/>
	</start>}

append_if [have_spec imx53] config {
	<start name="input_drv">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Input"/></provides>
		<config/>
	</start> }

append_if [have_spec ps2] config {
	<start name="ps2_drv">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Input"/></provides>
	</start>}

append_if [expr ![have_spec ps2] && [have_spec usb]] config {
	<start name="usb_drv">
		<resource name="RAM" quantum="12M"/>
		<provides><service name="Input"/></provides>
		<config ehci="yes" uhci="yes" xhci="no"> <hid/> </config>
	</start> }

append config {
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Timer"/></provides>
	</start>
	<start name="nitpicker">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Nitpicker"/></provides>
		<config>
			<domain name="" layer="2" />
			<policy label="" domain=""/>
			<report pointer="yes" />
		</config>
		<route>
			<service name="Report"> <child name="report_rom"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>
	<start name="report_rom">
		<resource name="RAM" quantum="2M"/>
		<provides> <service name="ROM" />
		           <service name="Report" /> </provides>
		<config>
			<rom>
				<policy label="decorator -> pointer"
				       report="nitpicker -> pointer"/>
				<policy label="decorator -> window_layout"
				       report="test-decorator_stress -> window_layout"/>
			</rom>
		</config>
	</start>
	<start name="test-decorator_stress">
		<resource name="RAM" quantum="2M"/>
		<route>
			<service name="Report"> <child name="report_rom"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>
	<start name="decorator">
		<resource name="RAM" quantum="8M"/>
		<route>
			<service name="ROM">
				<if-arg key="label" value="pointer" />
				<child name="report_rom" />
			</service>
			<service name="ROM">
				<if-arg key="label" value="window_layout" />
				<child name="report_rom" />
			</service>
			<service name="Report"> <child name="report_rom"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>
</config>}

install_config $config


#
# Boot modules
#

# generic modules
set boot_modules {
	core init
	timer
	decorator
	nitpicker report_rom
	test-decorator_stress
	ld.lib.so libc.lib.so libm.lib.so
}

# platform-specific modules
append_platform_drv_boot_modules

lappend_if [have_spec linux]            boot_modules fb_sdl
lappend_if [have_spec ps2]              boot_modules ps2_drv
lappend_if [have_spec framebuffer]      boot_modules fb_drv
lappend_if [have_spec usb]              boot_modules usb_drv
lappend_if [have_spec gpio]             boot_modules gpio_drv
lappend_if [have_spec imx53]            boot_modules input_drv

build_boot_image $boot_modules

append qemu_args " -m 256 "

run_genode_until forever
