#
# \brief  Test pong
# \author Josef Soentgen
# \date   2013-01-06
#

#
# Build
#

if {[have_spec hw_odroid_xu]} {
	puts "Run script does not support this platform."
	exit 0
}

set build_components {
	core init
	drivers/timer drivers/nic
	test/lwip/pingpong/server
}

lappend_if [expr [have_spec omap4] || [have_spec arndale]] build_components drivers/usb
lappend_if [have_spec gpio]             build_components drivers/gpio

source ${genode_dir}/repos/base/run/platform_drv.inc
append_platform_drv_build_components

build $build_components

create_boot_directory

#
# Generate config
#

set config {
<config verbose="yes">
	<parent-provides>
		<service name="ROM"/>
		<service name="RAM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="CAP"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
		<service name="SIGNAL"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Timer"/> </provides>
	</start>
	<start name="test-ping_server_libc_lwip">
		<resource name="RAM" quantum="16M"/>
		<config>
			<argv verbose="0" listenip="0.0.0.0" />
			<libc stdout="/dev/log" stderr="/dev/log">
				<vfs> <dir name="dev"> <log/> </dir> </vfs>
			</libc>
		</config>
	</start> }

append_if [have_spec gpio] config {
	<start name="gpio_drv">
		<resource name="RAM" quantum="4M"/>
		<provides><service name="Gpio"/></provides>
		<config/>
	</start>}

append_if [expr [have_spec omap4] || [have_spec arndale]] config {
	<start name="usb_drv" priority="-1">
		<resource name="RAM" quantum="12M"/>
		<provides>
			<service name="Nic"/>
		</provides>
		<config ehci="yes">
			<nic mac="02:00:00:00:01:01" />
		</config>
	</start>}

append_if [expr ![have_spec omap4] && ![have_spec arndale]] config {
	<start name="nic_drv">
		<resource name="RAM" quantum="4M"/>
		<provides><service name="Nic"/></provides>
	</start>}

append_platform_drv_config

append config {
</config>
}

install_config $config

#
# Boot modules
#

# generic modules
set boot_modules {
	core init timer
	ld.lib.so libc.lib.so lwip.lib.so
	test-ping_server_libc_lwip
}

# platform-specific modules
lappend_if [expr [have_spec omap4] || [have_spec arndale]]   boot_modules usb_drv
lappend_if [expr ![have_spec omap4] && ![have_spec arndale]] boot_modules nic_drv
lappend_if [have_spec gpio]                                           boot_modules gpio_drv

append_platform_drv_boot_modules

build_boot_image $boot_modules

#
# Execute test case
#

# qemu config
append qemu_args " -m 128 -nographic "

append_if [have_spec x86]     qemu_args " -net nic,model=e1000 "
append_if [have_spec lan9118] qemu_args " -net nic,model=lan9118 "

append qemu_args " -net user "

run_genode_until forever

# vi: set ft=tcl :
