diff -r f6df37e9f744 drivers/usb/dwc3/core.c
--- a/drivers/usb/dwc3/core.c	Mon Apr 29 17:06:54 2013 +0200
+++ b/drivers/usb/dwc3/core.c	Mon Apr 29 17:08:04 2013 +0200
@@ -480,7 +480,8 @@
 		goto err0;
 	}
 
-	mode = DWC3_MODE(dwc->hwparams.hwparams0);
+	/* force host mode which is needed for Exynos5 */
+	mode = DWC3_MODE_HOST;
 
 	switch (mode) {
 	case DWC3_MODE_DEVICE:
