set use_qemu [have_include "power_on/qemu"]

#
# Build
#

set build_components {
	core init timer
	drivers/usb_host
	drivers/usb_block
	server/report_rom
	test/block/client
	test/block/bench
}

lappend_if [have_spec gpio] build_components drivers/gpio

source ${genode_dir}/repos/base/run/platform_drv.inc
append_platform_drv_build_components

build $build_components

create_boot_directory

#
# Generate config
#

set config {
<config verbose="yes">
	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>

	<default caps="100"/>}

append_platform_drv_config

append_if [have_spec gpio] config "
	<start name=\"[gpio_drv]\">
		<resource name=\"RAM\" quantum=\"4M\"/>
		<provides><service name=\"Gpio\"/></provides>
		<config/>
	</start>"

append config {
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Timer"/> </provides>
	</start>
	<start name="report_rom">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Report"/> <service name="ROM"/> </provides>
		<config verbose="yes">
			<default-policy report="usb_drv -> devices"/>
		</config>
	</start>
	<start name="usb_drv" caps="120"> }
append config "<binary name=\"[usb_host_drv_binary]\"/>"
append config {
		<resource name="RAM" quantum="12M"/>
		<provides> <service name="Usb"/> </provides>
		<config>
			<report devices="no"/>}
append_if [expr !$use_qemu] config  {
			<!--
				The order is important because only the first policy is
				picked up - an entry may be moved to the front to test the
				corresponding device.
			 -->
			<!-- zte open c needs interface="3" -->
			<default-policy vendor_id="0x19d2" product_id="0x1350"/>
			<!-- kingston -->
			<default-policy vendor_id="0x0951" product_id="0x1666"/>
			<!-- voyager gt stick -->
			<default-policy vendor_id="0x1b1c" product_id="0x1a09"/>
			<!-- usb3 hdd adapter -->
			<default-policy vendor_id="0x174c" product_id="0x5106"/>
			<!-- lenovo disc -->
			<default-policy vendor_id="0x0984" product_id="0x0066"/>
}
append_if $use_qemu config {
			<default-policy bus="0x001" dev="0x002"/> }
append config {
		</config>
		<route>
			<service name="Report"> <child name="report_rom"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>
	<start name="usb_block_drv">
		<resource name="RAM" quantum="4M"/>
		<provides> <service name="Block"/> </provides>
		<config report="yes"/>
		<route>
			<service name="Usb"> <child name="usb_drv"/> </service>
			<service name="Report"> <child name="report_rom"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>
	<start name="test-usb">
		<resource name="RAM" quantum="128M"/>
		<binary name="test-block-bench"/>
		<!--binary name="test-block-client"/-->
		<config>
			<libc stdout="/dev/log">
				<vfs> <dir name="dev"> <log/> </dir> </vfs>
			</libc>
		</config>
		<route>
			<service name="Block"> <child name="usb_block_drv"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>
</config>}

install_config $config

#
# Boot modules
#

# generic modules
set boot_modules {
	core init timer report_rom usb_block_drv
	test-block-client test-block-bench
	ld.lib.so
}

append boot_modules [usb_host_drv_binary]
lappend_if [have_spec gpio] boot_modules [gpio_drv]

append_platform_drv_boot_modules

build_boot_image $boot_modules

#
# Execute test case
#
set disk_image "bin/test.img"
set cmd "dd if=/dev/zero of=$disk_image bs=1M count=16"
if {$use_qemu} {
	puts "creating disk image:\n$cmd"
	catch { exec sh -c $cmd }
}

#
# Qemu opts for EHCI
#
append qemu_args "  -nographic -M pc -boot order=d "
append qemu_args " -drive if=none,id=disk,file=$disk_image,format=raw "
append qemu_args " -device usb-ehci,id=ehci -device usb-storage,bus=ehci.0,drive=disk "

run_genode_until {.*child "test-usb" exited with exit value 0.*} 100
