(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)

  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 191)
    (zones 0)
    (modules 59)
    (nets 42)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.8)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./"))
  )

  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C1-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C2-Pad2)")
  (net 6 "Net-(C3-Pad1)")
  (net 7 "Net-(C3-Pad2)")
  (net 8 "Net-(C4-Pad1)")
  (net 9 "Net-(C10-Pad1)")
  (net 10 "Net-(C5-Pad1)")
  (net 11 "Net-(C5-Pad2)")
  (net 12 "Net-(C6-Pad1)")
  (net 13 "Net-(C12-Pad2)")
  (net 14 "Net-(C7-Pad1)")
  (net 15 "Net-(C11-Pad2)")
  (net 16 Earth)
  (net 17 "Net-(C8a1-Pad2)")
  (net 18 "Net-(C8b1-Pad2)")
  (net 19 "Net-(C9a1-Pad1)")
  (net 20 "Net-(C9a1-Pad2)")
  (net 21 "Net-(C9b1-Pad2)")
  (net 22 "Net-(C11-Pad1)")
  (net 23 "Net-(C12-Pad1)")
  (net 24 "Net-(C13-Pad1)")
  (net 25 +9V)
  (net 26 "Net-(BT1-Pad2)")
  (net 27 "Net-(D6-Pad1)")
  (net 28 "Net-(D6-Pad2)")
  (net 29 "Net-(Q1-Pad3)")
  (net 30 "Net-(Q2-Pad3)")
  (net 31 "Net-(Q3-Pad3)")
  (net 32 "Net-(Q4-Pad3)")
  (net 33 "Net-(R23-Pad1)")
  (net 34 "Net-(J3-Pad2)")
  (net 35 "Net-(R25-Pad3)")
  (net 36 "Net-(R2-Pad2)")
  (net 37 "Net-(C14-Pad2)")
  (net 38 "Net-(R26-Pad2)")
  (net 39 "Net-(J1-PadT)")
  (net 40 "Net-(S1-Pad3)")
  (net 41 "Net-(J2-PadT)")

  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.8)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +9V)
    (add_net Earth)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(BT1-Pad2)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8a1-Pad2)")
    (add_net "Net-(C8b1-Pad2)")
    (add_net "Net-(C9a1-Pad1)")
    (add_net "Net-(C9a1-Pad2)")
    (add_net "Net-(C9b1-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(J1-PadT)")
    (add_net "Net-(J2-PadT)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(Q4-Pad3)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R23-Pad1)")
    (add_net "Net-(R25-Pad3)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(S1-Pad3)")
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED121E)
    (at 157.099 92.71 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D863A5)
    (fp_text reference R8 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 33k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 "Net-(C11-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 "Net-(R25-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_THT:SW_CuK_JS202011CQN_DPDT_Straight (layer F.Cu) (tedit 5C63695E) (tstamp 5C636021)
    (at 145.923 91.567 90)
    (descr "CuK sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf")
    (tags "switch DPDT")
    (path /5C53C33E)
    (fp_text reference SW1 (at 2.75 -1.6 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_DPDT_x2 (at 3 5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -0.35) (end -2 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -2.25 4.25) (end -2.25 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.25 4.25) (end -2.25 4.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.25 -0.95) (end 7.25 4.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.95) (end 7.25 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 -0.75) (end -2.4 0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.2 -0.75) (end -2.4 -0.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.1 3.75) (end 5.9 3.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.1 -0.45) (end 7.1 3.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.9 -0.45) (end 7.1 -0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.1 3.75) (end -0.9 3.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.1 -0.45) (end -2.1 3.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.9 -0.45) (end -2.1 -0.45) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2 1.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2 3.65) (end -2 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 7 3.65) (end -2 3.65) (layer F.Fab) (width 0.1))
    (fp_line (start 7 -0.35) (end 7 3.65) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.35) (end 7 -0.35) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(C9a1-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(C11-Pad1)"))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(C9b1-Pad2)"))
    (pad 4 thru_hole circle (at 0 3.3 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(C8a1-Pad2)"))
    (pad 5 thru_hole circle (at 2.5 3.3 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(R25-Pad3)"))
    (pad 6 thru_hole circle (at 5 3.3 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(C8b1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_CuK_JS202011CQN_DPDT_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_THT:3PDT (layer F.Cu) (tedit 570516D6) (tstamp 5C5BAC0E)
    (at 166.243 117.348)
    (path /5C539AEE)
    (fp_text reference S1 (at 0 7.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SWITCH-3PDT (at 0 -7.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 -8.6) (end 9.8 -8.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 9.8 -8.6) (end 9.7 -8.6) (layer F.SilkS) (width 0.1))
    (fp_line (start -8.6 8.6) (end -9.8 8.6) (layer F.SilkS) (width 0.1))
    (fp_line (start -9.8 8.6) (end -9.8 0) (layer F.SilkS) (width 0.1))
    (fp_line (start -9.8 0) (end -9.8 -8.6) (layer F.SilkS) (width 0.1))
    (fp_line (start -9.8 -8.6) (end -8.6 -8.6) (layer F.SilkS) (width 0.1))
    (fp_line (start -8.6 -8.6) (end 0 -8.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 9.8 -8.6) (end 9.8 0) (layer F.SilkS) (width 0.1))
    (fp_line (start 9.8 0) (end 9.8 8.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 9.8 8.6) (end 0 8.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 0 8.6) (end -8.6 8.6) (layer F.SilkS) (width 0.1))
    (pad 5 thru_hole rect (at 0 0) (size 3.2 2) (drill oval 2.8 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 Earth))
    (pad 1 thru_hole rect (at -5.3 -4.7) (size 3.2 2) (drill oval 2.8 0.9525) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(R2-Pad2)"))
    (pad 2 thru_hole rect (at -5.3 0) (size 3.2 2) (drill oval 2.8 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J1-PadT)"))
    (pad 3 thru_hole rect (at -5.3 4.7) (size 3.2 2) (drill oval 2.8 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(S1-Pad3)"))
    (pad 4 thru_hole rect (at 0 -4.7) (size 3.2 2) (drill oval 2.8 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(D6-Pad1)"))
    (pad 6 thru_hole rect (at 0 4.7) (size 3.2 2) (drill oval 2.8 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 Earth))
    (pad 7 thru_hole rect (at 5.3 -4.7) (size 3.2 2) (drill oval 2.8 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(R26-Pad2)"))
    (pad 8 thru_hole rect (at 5.3 0) (size 3.2 2) (drill oval 2.8 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(J2-PadT)"))
    (pad 9 thru_hole rect (at 5.3 4.7) (size 3.2 2) (drill oval 2.8 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(S1-Pad3)"))
    (model ${KIPRJMOD}/3D/3PDT.step
      (offset (xyz -9 -6.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/3D/HammondBB.step
      (offset (xyz 0 34.5 18))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 180))
    )
  )

  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF) (tstamp 59ED11E7)
    (at 201.295 72.517)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (path /59D5E492)
    (fp_text reference Q4 (at 2.54 -3.56 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BC550C (at 2.54 2.79) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.74 1.85) (end 4.34 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 1.75) (end 4.3 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.01 -2.73) (end 6.09 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.01 -2.73) (end -1.01 2.01) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.09 2.01) (end 6.09 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.09 2.01) (end -1.01 2.01) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 2.54 0) (end 0.74 1.85) (angle 20) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.6) (angle -65) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.6) (angle 65) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.48) (angle 135) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.54 0) (end 2.54 -2.48) (angle -135) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.54 0) (end 4.34 1.85) (angle -20) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(Q4-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module Kicad_GSM_Footprint:SolderWirePad_2x_1-2mmDrill (layer F.Cu) (tedit 59EE6AF5) (tstamp 59EE6B9E)
    (at 125.603 101.219)
    (path /59E1758A)
    (fp_text reference BT1 (at 0 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 9V (at 0.635 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at -1.905 0) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole circle (at 1.905 0) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 26 "Net-(BT1-Pad2)"))
  )

  (module Kicad_GSM_Footprint:SolderWirePad_3x_1-2mmDrill (layer F.Cu) (tedit 59EE6176) (tstamp 59EE6345)
    (at 126.873 108.204 180)
    (path /59E13C16)
    (fp_text reference J3 (at 0 -3.81 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Jack-DC (at 1.27 3.81 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at -3.81 0 180) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 37 "Net-(C14-Pad2)"))
    (pad 3 thru_hole circle (at 3.81 0 180) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 26 "Net-(BT1-Pad2)"))
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1299)
    (at 166.497 98.171)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59EB7B94)
    (fp_text reference R28 (at 3.81 -1.86) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3.3k (at 3.81 1.86) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 +9V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0617_L17.0mm_D6.0mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1293)
    (at 154.813 101.092 180)
    (descr "Resistor, Axial_DIN0617 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0617 series Axial Horizontal pin pitch 20.32mm 2W length 17mm diameter 6mm")
    (path /59EA3323)
    (fp_text reference R27 (at 10.16 -4.06 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100 (at 10.16 4.06 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.66 -3) (end 1.66 3) (layer F.Fab) (width 0.1))
    (fp_line (start 1.66 3) (end 18.66 3) (layer F.Fab) (width 0.1))
    (fp_line (start 18.66 3) (end 18.66 -3) (layer F.Fab) (width 0.1))
    (fp_line (start 18.66 -3) (end 1.66 -3) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 20.32 0) (end 18.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -3.06) (end 1.6 3.06) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 3.06) (end 18.72 3.06) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.72 3.06) (end 18.72 -3.06) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.72 -3.06) (end 1.6 -3.06) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.38 0) (end 1.6 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.94 0) (end 18.72 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -3.35) (end -1.45 3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 3.35) (end 21.8 3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 21.8 3.35) (end 21.8 -3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 21.8 -3.35) (end -1.45 -3.35) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 +9V))
    (pad 2 thru_hole oval (at 20.32 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0617_L17.0mm_D6.0mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Kicad_GSM_Footprint:POT (layer F.Cu) (tedit 56F58C9D) (tstamp 59ED128D)
    (at 112.649 65.913 180)
    (path /59D9398C)
    (fp_text reference R26 (at -1.27 -2.54 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 2.54 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -1.27) (end -3.81 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.81 1.27) (end 3.81 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 1.27) (end 3.81 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 -1.27) (end -3.81 -1.27) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(R26-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 Earth))
  )

  (module Kicad_GSM_Footprint:POT (layer F.Cu) (tedit 56F58C9D) (tstamp 59ED1286)
    (at 151.892 65.913)
    (path /59D866C7)
    (fp_text reference R25 (at -1.27 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -1.27) (end -3.81 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.81 1.27) (end 3.81 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 1.27) (end 3.81 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 -1.27) (end -3.81 -1.27) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(C9a1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C3-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(R25-Pad3)"))
  )

  (module Kicad_GSM_Footprint:POT (layer F.Cu) (tedit 56F58C9D) (tstamp 59ED127F)
    (at 197.866 65.913 180)
    (path /59D7C9EC)
    (fp_text reference R24 (at -1.27 -2.54 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 2.54 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -1.27) (end -3.81 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.81 1.27) (end 3.81 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 1.27) (end 3.81 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 -1.27) (end -3.81 -1.27) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C5-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(R23-Pad1)"))
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1278)
    (at 191.77 68.707 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7CA93)
    (fp_text reference R23 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 "Net-(R23-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1272)
    (at 206.375 68.707 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7C852)
    (fp_text reference R22 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120 (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 "Net-(Q4-Pad3)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED126C)
    (at 189.23 68.707 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7E756)
    (fp_text reference R21 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 31 "Net-(Q3-Pad3)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1266)
    (at 186.69 68.707 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7E4FA)
    (fp_text reference R20 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(C12-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1260)
    (at 186.69 71.247)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7CD55)
    (fp_text reference R19 (at 3.81 -1.86) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.86) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(C12-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED125A)
    (at 181.356 94.996 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7DEF4)
    (fp_text reference R18 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 +9V))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1254)
    (at 184.277 83.947)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7D143)
    (fp_text reference R17 (at 3.81 -1.86) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470k (at 3.81 1.86) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 "Net-(C12-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED124E)
    (at 171.958 68.707 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7FAAC)
    (fp_text reference R16 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1248)
    (at 169.418 83.947)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7FA7C)
    (fp_text reference R15 (at 3.81 -1.86) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470k (at 3.81 1.86) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 "Net-(C11-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1242)
    (at 203.835 68.707 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7BC56)
    (fp_text reference R14 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED123C)
    (at 203.835 91.313 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7B711)
    (fp_text reference R13 (at 3.81 -1.86 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.86 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 +9V))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1236)
    (at 171.958 71.247)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7FA75)
    (fp_text reference R12 (at 3.81 -1.86) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.86) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1230)
    (at 166.497 94.996 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7FA9F)
    (fp_text reference R11 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 +9V))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED122A)
    (at 174.498 68.707 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7FAB3)
    (fp_text reference R10 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 30 "Net-(Q2-Pad3)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1224)
    (at 196.215 88.519)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7BB68)
    (fp_text reference R9 (at 3.81 -1.86) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470k (at 3.81 1.86) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1218)
    (at 130.048 85.979 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D91739)
    (fp_text reference R7 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 430k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 +9V))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1212)
    (at 127.508 85.979 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D92E3C)
    (fp_text reference R6 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 +9V))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 5C64077C)
    (at 166.243 68.326 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D8E71F)
    (fp_text reference R5 (at 3.81 -1.86 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22k (at 3.81 1.86 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 Earth))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(C9a1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1206)
    (at 132.588 68.707 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D92708)
    (fp_text reference R4 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3k3 (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED1200)
    (at 130.048 68.707 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D91E8D)
    (fp_text reference R3 (at 3.81 -1.86 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 3.81 1.86 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 Earth))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59ED11FA)
    (at 206.375 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (path /59D7BFBD)
    (fp_text reference R2 (at 3.81 -1.86 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 33k (at 3.81 1.86 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -0.86) (end 1.95 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 0.86) (end 5.67 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 0.86) (end 5.67 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.67 -0.86) (end 1.95 -0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.88 0) (end 1.95 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.74 0) (end 5.67 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.15) (end -0.95 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.15) (end 8.6 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 1.15) (end 8.6 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.6 -1.15) (end -0.95 -1.15) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 5995936A) (tstamp 59ED11A9)
    (at 165.1 103.378)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (path /59EB5D9D)
    (fp_text reference D6 (at 1.27 -3.96) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "LED 1.8V" (at 1.27 3.96) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.27 0) (end -1.23 -1.469694) (angle 299.1) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end -1.29 -1.54483) (angle 148.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -1.29 1.54483) (angle -148.9) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.23 -1.469694) (end -1.23 1.469694) (layer F.Fab) (width 0.1))
    (fp_line (start -1.29 -1.545) (end -1.29 1.545) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.95 -3.25) (end -1.95 3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 3.25) (end 4.5 3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.25) (end 4.5 -3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 -3.25) (end -1.95 -3.25) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.2)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5921392F) (tstamp 59ED11A3)
    (at 127.508 88.773 270)
    (descr "D, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (path /59E92029)
    (fp_text reference D5 (at 1.27 -2.690635 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1N4001 (at 1.27 3.579635 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at -2.390635 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.27 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 0) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.397 1.28) (end 1.397 2.169) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.397 1.7245) (end 1.989667 1.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.989667 1.28) (end 1.989667 2.169) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.989667 2.169) (end 1.397 1.7245) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.95) (end -1.7 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.95) (end 3.95 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.95 1.95) (end 3.95 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.95 -1.95) (end -1.7 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 1.35 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 0 0) (end 1.257516 -1.1) (angle -276.1) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 +9V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(C14-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_KathodeUp (layer F.Cu) (tedit 5921392F) (tstamp 59ED119D)
    (at 184.277 91.313)
    (descr "D, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (path /59D7D8BD)
    (fp_text reference D4 (at 1.27 -2.690635) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1N914 (at 1.27 3.579635) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at -1.8 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.27 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 0) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.397 1.28) (end 1.397 2.169) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.397 1.7245) (end 1.989667 1.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.989667 1.28) (end 1.989667 2.169) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.989667 2.169) (end 1.397 1.7245) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -1.95) (end -1.45 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 1.95) (end 4.2 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.2 1.95) (end 4.2 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.2 -1.95) (end -1.45 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.54 0) (end 3.89 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.54 0) (end 1.282484 -1.1) (angle 276.1) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(C12-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P2.54mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5921392F) (tstamp 59ED1197)
    (at 186.817 87.249 180)
    (descr "D, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (path /59D7D7EC)
    (fp_text reference D3 (at 1.27 -2.690635 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1N914 (at 1.27 3.579635 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at -2.390635 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.27 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 0) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.397 1.28) (end 1.397 2.169) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.397 1.7245) (end 1.989667 1.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.989667 1.28) (end 1.989667 2.169) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.989667 2.169) (end 1.397 1.7245) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.95) (end -1.7 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.95) (end 3.95 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.95 1.95) (end 3.95 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.95 -1.95) (end -1.7 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 1.35 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 0 0) (end 1.257516 -1.1) (angle -276.1) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_KathodeUp (layer F.Cu) (tedit 5921392F) (tstamp 59ED1191)
    (at 169.418 91.44)
    (descr "D, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (path /59D7FA98)
    (fp_text reference D2 (at 1.27 -2.690635) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1N914 (at 1.27 3.579635) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at -1.8 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.27 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 0) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.397 1.28) (end 1.397 2.169) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.397 1.7245) (end 1.989667 1.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.989667 1.28) (end 1.989667 2.169) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.989667 2.169) (end 1.397 1.7245) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -1.95) (end -1.45 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 1.95) (end 4.2 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.2 1.95) (end 4.2 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.2 -1.95) (end -1.45 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.54 0) (end 3.89 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.54 0) (end 1.282484 -1.1) (angle 276.1) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(C11-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P2.54mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5921392F) (tstamp 59ED118B)
    (at 171.958 87.376 180)
    (descr "D, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (path /59D7FA91)
    (fp_text reference D1 (at 1.27 -2.690635 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1N914 (at 1.27 3.579635 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at -2.390635 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.27 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 0) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.397 1.28) (end 1.397 2.169) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.397 1.7245) (end 1.989667 1.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.989667 1.28) (end 1.989667 2.169) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.989667 2.169) (end 1.397 1.7245) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.95) (end -1.7 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.95) (end 3.95 1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.95 1.95) (end 3.95 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.95 -1.95) (end -1.7 -1.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 1.35 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 0 0) (end 1.257516 -1.1) (angle -276.1) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D13.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59ED1185)
    (at 116.713 88.773 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=13mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 13mm Electrolytic Capacitor")
    (path /59E9510F)
    (fp_text reference C14 (at 2.5 -7.81 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470µF (at 2.5 7.81 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 2.5 0) (end 9 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 9.09 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 0) (end -1.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 -0.9) (end -2.3 0.9) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -6.55) (end 2.5 6.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 -6.55) (end 2.54 6.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.58 -6.55) (end 2.58 6.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.62 -6.549) (end 2.62 6.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.66 -6.549) (end 2.66 6.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.7 -6.547) (end 2.7 6.547) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.74 -6.546) (end 2.74 6.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.78 -6.545) (end 2.78 6.545) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.82 -6.543) (end 2.82 6.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.86 -6.541) (end 2.86 6.541) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.9 -6.538) (end 2.9 6.538) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.94 -6.536) (end 2.94 6.536) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.98 -6.533) (end 2.98 6.533) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.02 -6.53) (end 3.02 6.53) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.06 -6.527) (end 3.06 6.527) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.1 -6.523) (end 3.1 6.523) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.14 -6.519) (end 3.14 6.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.18 -6.515) (end 3.18 6.515) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.221 -6.511) (end 3.221 6.511) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.261 -6.507) (end 3.261 6.507) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.301 -6.502) (end 3.301 6.502) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.341 -6.497) (end 3.341 6.497) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.381 -6.491) (end 3.381 6.491) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.421 -6.486) (end 3.421 6.486) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.461 -6.48) (end 3.461 6.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.501 -6.474) (end 3.501 6.474) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.541 -6.468) (end 3.541 6.468) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.581 -6.461) (end 3.581 6.461) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.621 -6.455) (end 3.621 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.621 1.38) (end 3.621 6.455) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.661 -6.448) (end 3.661 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.661 1.38) (end 3.661 6.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.701 -6.44) (end 3.701 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.701 1.38) (end 3.701 6.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.741 -6.433) (end 3.741 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.741 1.38) (end 3.741 6.433) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.781 -6.425) (end 3.781 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.781 1.38) (end 3.781 6.425) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.821 -6.417) (end 3.821 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.821 1.38) (end 3.821 6.417) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.861 -6.409) (end 3.861 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.861 1.38) (end 3.861 6.409) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.901 -6.4) (end 3.901 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.901 1.38) (end 3.901 6.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.941 -6.391) (end 3.941 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.941 1.38) (end 3.941 6.391) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.981 -6.382) (end 3.981 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.981 1.38) (end 3.981 6.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.021 -6.373) (end 4.021 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.021 1.38) (end 4.021 6.373) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.061 -6.363) (end 4.061 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.061 1.38) (end 4.061 6.363) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.101 -6.353) (end 4.101 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.101 1.38) (end 4.101 6.353) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.141 -6.343) (end 4.141 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.141 1.38) (end 4.141 6.343) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.181 -6.333) (end 4.181 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.181 1.38) (end 4.181 6.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.221 -6.322) (end 4.221 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.221 1.38) (end 4.221 6.322) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.261 -6.311) (end 4.261 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.261 1.38) (end 4.261 6.311) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.301 -6.3) (end 4.301 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.301 1.38) (end 4.301 6.3) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.341 -6.288) (end 4.341 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.341 1.38) (end 4.341 6.288) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.381 -6.277) (end 4.381 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.381 1.38) (end 4.381 6.277) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.421 -6.265) (end 4.421 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.421 1.38) (end 4.421 6.265) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.461 -6.252) (end 4.461 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.461 1.38) (end 4.461 6.252) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.501 -6.24) (end 4.501 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.501 1.38) (end 4.501 6.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.541 -6.227) (end 4.541 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.541 1.38) (end 4.541 6.227) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.581 -6.214) (end 4.581 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.581 1.38) (end 4.581 6.214) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.621 -6.2) (end 4.621 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.621 1.38) (end 4.621 6.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.661 -6.186) (end 4.661 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.661 1.38) (end 4.661 6.186) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.701 -6.172) (end 4.701 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.701 1.38) (end 4.701 6.172) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.741 -6.158) (end 4.741 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.741 1.38) (end 4.741 6.158) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.781 -6.144) (end 4.781 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.781 1.38) (end 4.781 6.144) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.821 -6.129) (end 4.821 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.821 1.38) (end 4.821 6.129) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.861 -6.113) (end 4.861 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.861 1.38) (end 4.861 6.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.901 -6.098) (end 4.901 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.901 1.38) (end 4.901 6.098) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.941 -6.082) (end 4.941 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.941 1.38) (end 4.941 6.082) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.981 -6.066) (end 4.981 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.981 1.38) (end 4.981 6.066) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.021 -6.05) (end 5.021 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.021 1.38) (end 5.021 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.061 -6.033) (end 5.061 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.061 1.38) (end 5.061 6.033) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.101 -6.016) (end 5.101 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.101 1.38) (end 5.101 6.016) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.141 -5.999) (end 5.141 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.141 1.38) (end 5.141 5.999) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.181 -5.981) (end 5.181 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.181 1.38) (end 5.181 5.981) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.221 -5.963) (end 5.221 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.221 1.38) (end 5.221 5.963) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.261 -5.945) (end 5.261 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.261 1.38) (end 5.261 5.945) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.301 -5.926) (end 5.301 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.301 1.38) (end 5.301 5.926) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.341 -5.907) (end 5.341 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.341 1.38) (end 5.341 5.907) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.381 -5.888) (end 5.381 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.381 1.38) (end 5.381 5.888) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.421 -5.868) (end 5.421 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.421 1.38) (end 5.421 5.868) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.461 -5.848) (end 5.461 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.461 1.38) (end 5.461 5.848) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.501 -5.828) (end 5.501 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.501 1.38) (end 5.501 5.828) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.541 -5.807) (end 5.541 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.541 1.38) (end 5.541 5.807) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.581 -5.786) (end 5.581 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.581 1.38) (end 5.581 5.786) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.621 -5.765) (end 5.621 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.621 1.38) (end 5.621 5.765) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.661 -5.743) (end 5.661 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.661 1.38) (end 5.661 5.743) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.701 -5.721) (end 5.701 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.701 1.38) (end 5.701 5.721) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.741 -5.699) (end 5.741 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.741 1.38) (end 5.741 5.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.781 -5.676) (end 5.781 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.781 1.38) (end 5.781 5.676) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.821 -5.653) (end 5.821 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.821 1.38) (end 5.821 5.653) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.861 -5.63) (end 5.861 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.861 1.38) (end 5.861 5.63) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.901 -5.606) (end 5.901 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.901 1.38) (end 5.901 5.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.941 -5.581) (end 5.941 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.941 1.38) (end 5.941 5.581) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.981 -5.557) (end 5.981 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.981 1.38) (end 5.981 5.557) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.021 -5.532) (end 6.021 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.021 1.38) (end 6.021 5.532) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.061 -5.506) (end 6.061 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.061 1.38) (end 6.061 5.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.101 -5.48) (end 6.101 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.101 1.38) (end 6.101 5.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.141 -5.454) (end 6.141 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.141 1.38) (end 6.141 5.454) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.181 -5.427) (end 6.181 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.181 1.38) (end 6.181 5.427) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.221 -5.4) (end 6.221 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.221 1.38) (end 6.221 5.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.261 -5.373) (end 6.261 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.261 1.38) (end 6.261 5.373) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.301 -5.345) (end 6.301 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.301 1.38) (end 6.301 5.345) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.341 -5.316) (end 6.341 -1.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.341 1.38) (end 6.341 5.316) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.381 -5.287) (end 6.381 5.287) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.421 -5.258) (end 6.421 5.258) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.461 -5.228) (end 6.461 5.228) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.501 -5.198) (end 6.501 5.198) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.541 -5.167) (end 6.541 5.167) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.581 -5.136) (end 6.581 5.136) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.621 -5.104) (end 6.621 5.104) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.661 -5.072) (end 6.661 5.072) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.701 -5.039) (end 6.701 5.039) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.741 -5.005) (end 6.741 5.005) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.781 -4.971) (end 6.781 4.971) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.821 -4.937) (end 6.821 4.937) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.861 -4.902) (end 6.861 4.902) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.901 -4.866) (end 6.901 4.866) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.941 -4.83) (end 6.941 4.83) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.981 -4.793) (end 6.981 4.793) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.021 -4.756) (end 7.021 4.756) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.061 -4.718) (end 7.061 4.718) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.101 -4.679) (end 7.101 4.679) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.141 -4.64) (end 7.141 4.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.181 -4.6) (end 7.181 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.221 -4.559) (end 7.221 4.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.261 -4.518) (end 7.261 4.518) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.301 -4.476) (end 7.301 4.476) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.341 -4.433) (end 7.341 4.433) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.381 -4.389) (end 7.381 4.389) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.421 -4.345) (end 7.421 4.345) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.461 -4.299) (end 7.461 4.299) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.501 -4.253) (end 7.501 4.253) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.541 -4.206) (end 7.541 4.206) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.581 -4.158) (end 7.581 4.158) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.621 -4.109) (end 7.621 4.109) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.661 -4.06) (end 7.661 4.06) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.701 -4.009) (end 7.701 4.009) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.741 -3.957) (end 7.741 3.957) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.781 -3.904) (end 7.781 3.904) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.821 -3.85) (end 7.821 3.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.861 -3.794) (end 7.861 3.794) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.901 -3.738) (end 7.901 3.738) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.941 -3.68) (end 7.941 3.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.981 -3.621) (end 7.981 3.621) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.021 -3.56) (end 8.021 3.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.061 -3.498) (end 8.061 3.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.101 -3.434) (end 8.101 3.434) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.141 -3.369) (end 8.141 3.369) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.181 -3.302) (end 8.181 3.302) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.221 -3.233) (end 8.221 3.233) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.261 -3.162) (end 8.261 3.162) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.301 -3.089) (end 8.301 3.089) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.341 -3.014) (end 8.341 3.014) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.381 -2.936) (end 8.381 2.936) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.421 -2.856) (end 8.421 2.856) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.461 -2.772) (end 8.461 2.772) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.501 -2.686) (end 8.501 2.686) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.541 -2.596) (end 8.541 2.596) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.581 -2.502) (end 8.581 2.502) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.621 -2.405) (end 8.621 2.405) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.661 -2.302) (end 8.661 2.302) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.701 -2.194) (end 8.701 2.194) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.741 -2.08) (end 8.741 2.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.781 -1.958) (end 8.781 1.958) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.821 -1.828) (end 8.821 1.828) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.861 -1.686) (end 8.861 1.686) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.901 -1.532) (end 8.901 1.532) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.941 -1.359) (end 8.941 1.359) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.981 -1.16) (end 8.981 1.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.021 -0.918) (end 9.021 0.918) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.061 -0.589) (end 9.061 0.589) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 0) (end -1.4 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.3 -0.9) (end -2.3 0.9) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.35 -6.85) (end -4.35 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.35 6.85) (end 9.35 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.35 6.85) (end 9.35 -6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.35 -6.85) (end -4.35 -6.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 +9V))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 "Net-(C14-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D13.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 59EBB35D) (tstamp 59ED117F)
    (at 178.435 77.597 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (path /59D7FA6E)
    (fp_text reference C13 (at 1.25 -2.31 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.1µF (at 1.25 2.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.05 -1.25) (end -1.05 1.25) (layer F.Fab) (width 0.15))
    (fp_line (start -1.05 1.25) (end 3.55 1.25) (layer F.Fab) (width 0.15))
    (fp_line (start 3.55 1.25) (end 3.55 -1.25) (layer F.Fab) (width 0.15))
    (fp_line (start 3.55 -1.25) (end -1.05 -1.25) (layer F.Fab) (width 0.15))
    (fp_line (start -1.11 -1.31) (end 3.61 -1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.11 1.31) (end 3.61 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.11 -1.31) (end -1.11 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.61 -1.31) (end 3.61 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.4 -1.5) (end -1.4 1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.4 1.5) (end 3.9 1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.9 1.5) (end 3.9 -1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.9 -1.5) (end -1.4 -1.5) (layer F.CrtYd) (width 0.15))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 597BC7C2) (tstamp 59ED1179)
    (at 184.277 80.01)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (path /59D7D1E6)
    (fp_text reference C12 (at 2.5 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470pF (at 2.5 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -2.25) (end -1.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 2.25) (end 6.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 2.25) (end 6.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -2.25) (end -1.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.16 -2.31) (end 6.16 -2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 -2.31) (end -1.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.16 -2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -2.6) (end -1.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 2.6) (end 6.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 2.6) (end 6.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 -2.6) (end -1.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 597BC7C2) (tstamp 59ED1173)
    (at 169.418 80.01)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (path /59D7FA83)
    (fp_text reference C11 (at 2.5 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470pF (at 2.5 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -2.25) (end -1.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 2.25) (end 6.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 2.25) (end 6.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -2.25) (end -1.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.16 -2.31) (end 6.16 -2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 -2.31) (end -1.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.16 -2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -2.6) (end -1.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 2.6) (end 6.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 2.6) (end 6.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 -2.6) (end -1.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C11-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 597BC7C2) (tstamp 59ED116D)
    (at 198.755 84.455)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (path /59D7B9C6)
    (fp_text reference C10 (at 2.5 -3.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470pF (at 2.5 3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -2.25) (end -1.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 2.25) (end 6.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 2.25) (end 6.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -2.25) (end -1.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.16 -2.31) (end 6.16 -2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 -2.31) (end -1.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.16 -2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -2.6) (end -1.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 2.6) (end 6.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 2.6) (end 6.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 -2.6) (end -1.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 597BC7C2) (tstamp 59ED1167)
    (at 136.144 89.281 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*8.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 8.5mm Capacitor")
    (path /59D8CDB4)
    (fp_text reference C9b1 (at 2.5 -5.56 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.01µF (at 2.5 5.56 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -4.25) (end -1.1 4.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 4.25) (end 6.1 4.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 4.25) (end 6.1 -4.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -4.25) (end -1.1 -4.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.16 -4.31) (end 6.16 -4.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 4.31) (end 6.16 4.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 -4.31) (end -1.16 4.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.16 -4.31) (end 6.16 4.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -4.6) (end -1.45 4.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 4.6) (end 6.45 4.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 4.6) (end 6.45 -4.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 -4.6) (end -1.45 -4.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C9a1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C9b1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 597BC7C2) (tstamp 59ED1161)
    (at 134.112 93.98)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (path /59D8CA79)
    (fp_text reference C9a1 (at 2.5 -4.06) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.004µF (at 2.5 4.06) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -2.75) (end -1.1 2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 2.75) (end 6.1 2.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 2.75) (end 6.1 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -2.75) (end -1.1 -2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.16 -2.81) (end 6.16 -2.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 2.81) (end 6.16 2.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 -2.81) (end -1.16 2.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.16 -2.81) (end 6.16 2.81) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -3.1) (end -1.45 3.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 3.1) (end 6.45 3.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 3.1) (end 6.45 -3.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 -3.1) (end -1.45 -3.1) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C9a1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C9a1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5C636DC9) (tstamp 5C640ABD)
    (at 166.243 82.677 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (path /59D8860E)
    (fp_text reference C8b1 (at 2.5 -3.56 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.0056µF (at 2.5 3.56 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -2.25) (end -1.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 2.25) (end 6.1 2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 2.25) (end 6.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -2.25) (end -1.1 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.16 -2.31) (end 6.16 -2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 -2.31) (end -1.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.16 -2.31) (end 6.16 2.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -2.6) (end -1.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 2.6) (end 6.45 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 2.6) (end 6.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 -2.6) (end -1.45 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 Earth))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C8b1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 597BC7C2) (tstamp 5C64086B)
    (at 166.243 75.184 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*8.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 8.5mm Capacitor")
    (path /59D87D85)
    (fp_text reference C8a1 (at 2.5 -5.56 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.01µF (at 2.5 5.56 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -4.25) (end -1.1 4.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 4.25) (end 6.1 4.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 4.25) (end 6.1 -4.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -4.25) (end -1.1 -4.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.16 -4.31) (end 6.16 -4.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 4.31) (end 6.16 4.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.16 -4.31) (end -1.16 4.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.16 -4.31) (end 6.16 4.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.45 -4.6) (end -1.45 4.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 4.6) (end 6.45 4.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 4.6) (end 6.45 -4.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.45 -4.6) (end -1.45 -4.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 Earth))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C8a1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59ED114F)
    (at 177.038 89.154 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (path /59D7FA8A)
    (fp_text reference C7 (at 1 -3.81 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1µF (at 1 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1 0) (end -1.30558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end -1.30558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end 3.30558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -2.55) (end 1 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -2.55) (end 1.04 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0.98) (end 1.04 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.08 -2.549) (end 1.08 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.08 0.98) (end 1.08 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.12 -2.548) (end 1.12 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.12 0.98) (end 1.12 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -2.546) (end 1.16 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 0.98) (end 1.16 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 -2.543) (end 1.2 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 0.98) (end 1.2 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 -2.539) (end 1.24 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 0.98) (end 1.24 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 -2.535) (end 1.28 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 0.98) (end 1.28 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 -2.531) (end 1.32 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 0.98) (end 1.32 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 -2.525) (end 1.36 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 0.98) (end 1.36 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -2.519) (end 1.4 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 0.98) (end 1.4 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 -2.513) (end 1.44 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 0.98) (end 1.44 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 -2.506) (end 1.48 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 0.98) (end 1.48 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 -2.498) (end 1.52 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 0.98) (end 1.52 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -2.489) (end 1.56 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 0.98) (end 1.56 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 -2.48) (end 1.6 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.98) (end 1.6 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 -2.47) (end 1.64 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 0.98) (end 1.64 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 -2.46) (end 1.68 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 0.98) (end 1.68 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 -2.448) (end 1.721 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 0.98) (end 1.721 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 -2.436) (end 1.761 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 0.98) (end 1.761 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 -2.424) (end 1.801 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 0.98) (end 1.801 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 -2.41) (end 1.841 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 0.98) (end 1.841 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 -2.396) (end 1.881 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 0.98) (end 1.881 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 -2.382) (end 1.921 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 0.98) (end 1.921 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 -2.366) (end 1.961 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 0.98) (end 1.961 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 -2.35) (end 2.001 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 0.98) (end 2.001 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 -2.333) (end 2.041 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 0.98) (end 2.041 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 -2.315) (end 2.081 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 0.98) (end 2.081 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 -2.296) (end 2.121 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 0.98) (end 2.121 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 -2.276) (end 2.161 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 0.98) (end 2.161 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 -2.256) (end 2.201 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 0.98) (end 2.201 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 -2.234) (end 2.241 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 0.98) (end 2.241 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 -2.212) (end 2.281 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 0.98) (end 2.281 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 -2.189) (end 2.321 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 0.98) (end 2.321 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 -2.165) (end 2.361 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 0.98) (end 2.361 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 -2.14) (end 2.401 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 0.98) (end 2.401 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 -2.113) (end 2.441 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 0.98) (end 2.441 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 -2.086) (end 2.481 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 0.98) (end 2.481 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 -2.058) (end 2.521 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 0.98) (end 2.521 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 -2.028) (end 2.561 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 0.98) (end 2.561 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 -1.997) (end 2.601 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 0.98) (end 2.601 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 -1.965) (end 2.641 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 0.98) (end 2.641 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 -1.932) (end 2.681 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 0.98) (end 2.681 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 -1.897) (end 2.721 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 0.98) (end 2.721 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 -1.861) (end 2.761 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 0.98) (end 2.761 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.801 -1.823) (end 2.801 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.801 0.98) (end 2.801 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.841 -1.783) (end 2.841 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.841 0.98) (end 2.841 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.881 -1.742) (end 2.881 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.881 0.98) (end 2.881 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.921 -1.699) (end 2.921 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.921 0.98) (end 2.921 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.961 -1.654) (end 2.961 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.961 0.98) (end 2.961 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.001 -1.606) (end 3.001 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.041 -1.556) (end 3.041 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.081 -1.504) (end 3.081 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.121 -1.448) (end 3.121 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.161 -1.39) (end 3.161 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.201 -1.327) (end 3.201 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.241 -1.261) (end 3.241 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.281 -1.189) (end 3.281 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.321 -1.112) (end 3.321 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.361 -1.028) (end 3.361 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.401 -0.934) (end 3.401 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.441 -0.829) (end 3.441 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.481 -0.707) (end 3.481 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.521 -0.559) (end 3.521 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.561 -0.354) (end 3.561 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 -2.85) (end -1.85 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 2.85) (end 3.85 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.85) (end 3.85 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.85) (end -1.85 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59ED1149)
    (at 191.897 89.154 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (path /59D7D2A1)
    (fp_text reference C6 (at 1 -3.81 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1µF (at 1 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1 0) (end -1.30558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end -1.30558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end 3.30558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -2.55) (end 1 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -2.55) (end 1.04 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0.98) (end 1.04 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.08 -2.549) (end 1.08 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.08 0.98) (end 1.08 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.12 -2.548) (end 1.12 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.12 0.98) (end 1.12 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -2.546) (end 1.16 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 0.98) (end 1.16 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 -2.543) (end 1.2 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 0.98) (end 1.2 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 -2.539) (end 1.24 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 0.98) (end 1.24 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 -2.535) (end 1.28 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 0.98) (end 1.28 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 -2.531) (end 1.32 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 0.98) (end 1.32 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 -2.525) (end 1.36 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 0.98) (end 1.36 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -2.519) (end 1.4 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 0.98) (end 1.4 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 -2.513) (end 1.44 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 0.98) (end 1.44 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 -2.506) (end 1.48 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 0.98) (end 1.48 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 -2.498) (end 1.52 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 0.98) (end 1.52 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -2.489) (end 1.56 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 0.98) (end 1.56 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 -2.48) (end 1.6 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.98) (end 1.6 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 -2.47) (end 1.64 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 0.98) (end 1.64 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 -2.46) (end 1.68 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 0.98) (end 1.68 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 -2.448) (end 1.721 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 0.98) (end 1.721 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 -2.436) (end 1.761 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 0.98) (end 1.761 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 -2.424) (end 1.801 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 0.98) (end 1.801 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 -2.41) (end 1.841 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 0.98) (end 1.841 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 -2.396) (end 1.881 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 0.98) (end 1.881 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 -2.382) (end 1.921 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 0.98) (end 1.921 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 -2.366) (end 1.961 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 0.98) (end 1.961 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 -2.35) (end 2.001 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 0.98) (end 2.001 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 -2.333) (end 2.041 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 0.98) (end 2.041 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 -2.315) (end 2.081 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 0.98) (end 2.081 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 -2.296) (end 2.121 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 0.98) (end 2.121 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 -2.276) (end 2.161 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 0.98) (end 2.161 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 -2.256) (end 2.201 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 0.98) (end 2.201 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 -2.234) (end 2.241 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 0.98) (end 2.241 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 -2.212) (end 2.281 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 0.98) (end 2.281 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 -2.189) (end 2.321 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 0.98) (end 2.321 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 -2.165) (end 2.361 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 0.98) (end 2.361 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 -2.14) (end 2.401 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 0.98) (end 2.401 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 -2.113) (end 2.441 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 0.98) (end 2.441 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 -2.086) (end 2.481 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 0.98) (end 2.481 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 -2.058) (end 2.521 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 0.98) (end 2.521 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 -2.028) (end 2.561 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 0.98) (end 2.561 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 -1.997) (end 2.601 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 0.98) (end 2.601 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 -1.965) (end 2.641 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 0.98) (end 2.641 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 -1.932) (end 2.681 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 0.98) (end 2.681 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 -1.897) (end 2.721 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 0.98) (end 2.721 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 -1.861) (end 2.761 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 0.98) (end 2.761 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.801 -1.823) (end 2.801 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.801 0.98) (end 2.801 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.841 -1.783) (end 2.841 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.841 0.98) (end 2.841 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.881 -1.742) (end 2.881 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.881 0.98) (end 2.881 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.921 -1.699) (end 2.921 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.921 0.98) (end 2.921 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.961 -1.654) (end 2.961 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.961 0.98) (end 2.961 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.001 -1.606) (end 3.001 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.041 -1.556) (end 3.041 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.081 -1.504) (end 3.081 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.121 -1.448) (end 3.121 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.161 -1.39) (end 3.161 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.201 -1.327) (end 3.201 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.241 -1.261) (end 3.241 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.281 -1.189) (end 3.281 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.321 -1.112) (end 3.321 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.361 -1.028) (end 3.361 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.401 -0.934) (end 3.401 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.441 -0.829) (end 3.441 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.481 -0.707) (end 3.481 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.521 -0.559) (end 3.521 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.561 -0.354) (end 3.561 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 -2.85) (end -1.85 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 2.85) (end 3.85 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.85) (end 3.85 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.85) (end -1.85 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 59EBB35D) (tstamp 59ED1143)
    (at 194.31 74.295 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (path /59D7CC75)
    (fp_text reference C5 (at 1.25 -2.31 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.1µF (at 1.25 2.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.05 -1.25) (end -1.05 1.25) (layer F.Fab) (width 0.15))
    (fp_line (start -1.05 1.25) (end 3.55 1.25) (layer F.Fab) (width 0.15))
    (fp_line (start 3.55 1.25) (end 3.55 -1.25) (layer F.Fab) (width 0.15))
    (fp_line (start 3.55 -1.25) (end -1.05 -1.25) (layer F.Fab) (width 0.15))
    (fp_line (start -1.11 -1.31) (end 3.61 -1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.11 1.31) (end 3.61 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.11 -1.31) (end -1.11 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.61 -1.31) (end 3.61 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.4 -1.5) (end -1.4 1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.4 1.5) (end 3.9 1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.9 1.5) (end 3.9 -1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.9 -1.5) (end -1.4 -1.5) (layer F.CrtYd) (width 0.15))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 59EBB35D) (tstamp 59ED113D)
    (at 198.755 77.851 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (path /59D7C93F)
    (fp_text reference C4 (at 1.25 -2.31 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.1µF (at 1.25 2.31 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.05 -1.25) (end -1.05 1.25) (layer F.Fab) (width 0.15))
    (fp_line (start -1.05 1.25) (end 3.55 1.25) (layer F.Fab) (width 0.15))
    (fp_line (start 3.55 1.25) (end 3.55 -1.25) (layer F.Fab) (width 0.15))
    (fp_line (start 3.55 -1.25) (end -1.05 -1.25) (layer F.Fab) (width 0.15))
    (fp_line (start -1.11 -1.31) (end 3.61 -1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.11 1.31) (end 3.61 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.11 -1.31) (end -1.11 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.61 -1.31) (end 3.61 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.4 -1.5) (end -1.4 1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.4 1.5) (end 3.9 1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.9 1.5) (end 3.9 -1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.9 -1.5) (end -1.4 -1.5) (layer F.CrtYd) (width 0.15))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 59EBB35D) (tstamp 59ED1137)
    (at 136.398 63.373)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (path /59D90B52)
    (fp_text reference C3 (at 1.25 -2.31) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.1µF (at 1.25 2.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.05 -1.25) (end -1.05 1.25) (layer F.Fab) (width 0.15))
    (fp_line (start -1.05 1.25) (end 3.55 1.25) (layer F.Fab) (width 0.15))
    (fp_line (start 3.55 1.25) (end 3.55 -1.25) (layer F.Fab) (width 0.15))
    (fp_line (start 3.55 -1.25) (end -1.05 -1.25) (layer F.Fab) (width 0.15))
    (fp_line (start -1.11 -1.31) (end 3.61 -1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.11 1.31) (end 3.61 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.11 -1.31) (end -1.11 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.61 -1.31) (end 3.61 1.31) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.4 -1.5) (end -1.4 1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.4 1.5) (end 3.9 1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.9 1.5) (end 3.9 -1.5) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.9 -1.5) (end -1.4 -1.5) (layer F.CrtYd) (width 0.15))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59ED1131)
    (at 123.317 74.93 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (path /59D937BB)
    (fp_text reference C2 (at 1 -3.81 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1µF (at 1 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1 0) (end -1.30558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end -1.30558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end 3.30558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1 0) (end 3.5 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -2.55) (end 1 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -2.55) (end 1.04 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0.98) (end 1.04 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.08 -2.549) (end 1.08 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.08 0.98) (end 1.08 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.12 -2.548) (end 1.12 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.12 0.98) (end 1.12 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -2.546) (end 1.16 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 0.98) (end 1.16 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 -2.543) (end 1.2 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 0.98) (end 1.2 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 -2.539) (end 1.24 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 0.98) (end 1.24 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 -2.535) (end 1.28 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 0.98) (end 1.28 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 -2.531) (end 1.32 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 0.98) (end 1.32 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 -2.525) (end 1.36 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 0.98) (end 1.36 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -2.519) (end 1.4 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 0.98) (end 1.4 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 -2.513) (end 1.44 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 0.98) (end 1.44 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 -2.506) (end 1.48 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 0.98) (end 1.48 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 -2.498) (end 1.52 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 0.98) (end 1.52 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -2.489) (end 1.56 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 0.98) (end 1.56 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 -2.48) (end 1.6 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.98) (end 1.6 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 -2.47) (end 1.64 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 0.98) (end 1.64 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 -2.46) (end 1.68 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 0.98) (end 1.68 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 -2.448) (end 1.721 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 0.98) (end 1.721 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 -2.436) (end 1.761 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 0.98) (end 1.761 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 -2.424) (end 1.801 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 0.98) (end 1.801 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 -2.41) (end 1.841 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 0.98) (end 1.841 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 -2.396) (end 1.881 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 0.98) (end 1.881 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 -2.382) (end 1.921 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 0.98) (end 1.921 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 -2.366) (end 1.961 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 0.98) (end 1.961 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 -2.35) (end 2.001 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 0.98) (end 2.001 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 -2.333) (end 2.041 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 0.98) (end 2.041 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 -2.315) (end 2.081 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 0.98) (end 2.081 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 -2.296) (end 2.121 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 0.98) (end 2.121 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 -2.276) (end 2.161 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 0.98) (end 2.161 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 -2.256) (end 2.201 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 0.98) (end 2.201 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 -2.234) (end 2.241 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 0.98) (end 2.241 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 -2.212) (end 2.281 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 0.98) (end 2.281 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 -2.189) (end 2.321 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 0.98) (end 2.321 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 -2.165) (end 2.361 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 0.98) (end 2.361 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 -2.14) (end 2.401 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 0.98) (end 2.401 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 -2.113) (end 2.441 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 0.98) (end 2.441 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 -2.086) (end 2.481 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 0.98) (end 2.481 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 -2.058) (end 2.521 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 0.98) (end 2.521 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 -2.028) (end 2.561 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 0.98) (end 2.561 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 -1.997) (end 2.601 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 0.98) (end 2.601 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 -1.965) (end 2.641 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 0.98) (end 2.641 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 -1.932) (end 2.681 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 0.98) (end 2.681 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 -1.897) (end 2.721 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 0.98) (end 2.721 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 -1.861) (end 2.761 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 0.98) (end 2.761 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.801 -1.823) (end 2.801 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.801 0.98) (end 2.801 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.841 -1.783) (end 2.841 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.841 0.98) (end 2.841 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.881 -1.742) (end 2.881 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.881 0.98) (end 2.881 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.921 -1.699) (end 2.921 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.921 0.98) (end 2.921 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.961 -1.654) (end 2.961 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.961 0.98) (end 2.961 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.001 -1.606) (end 3.001 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.041 -1.556) (end 3.041 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.081 -1.504) (end 3.081 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.121 -1.448) (end 3.121 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.161 -1.39) (end 3.161 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.201 -1.327) (end 3.201 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.241 -1.261) (end 3.241 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.281 -1.189) (end 3.281 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.321 -1.112) (end 3.321 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.361 -1.028) (end 3.361 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.401 -0.934) (end 3.401 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.441 -0.829) (end 3.441 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.481 -0.707) (end 3.481 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.521 -0.559) (end 3.521 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.561 -0.354) (end 3.561 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.85 -2.85) (end -1.85 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.85 2.85) (end 3.85 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 2.85) (end 3.85 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 -2.85) (end -1.85 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 597BC7C2) (tstamp 59ED112B)
    (at 203.835 78.105)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (path /59D7BD49)
    (fp_text reference C1 (at 1.25 -4.46) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10µF (at 1.25 4.46) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.25 0) (end -1.767482 -1.18) (angle 137.3) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.767482 1.18) (angle -137.3) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 4.267482 -1.18) (angle 42.7) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 4.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -3.2) (end 1.25 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -3.2) (end 1.29 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -3.2) (end 1.33 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -3.198) (end 1.37 3.198) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -3.197) (end 1.41 3.197) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -3.194) (end 1.45 3.194) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -3.192) (end 1.49 3.192) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -3.188) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 3.188) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -3.185) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 3.185) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -3.18) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 3.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -3.176) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 3.176) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -3.17) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 3.17) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -3.165) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 3.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -3.158) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 3.158) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -3.152) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 3.152) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -3.144) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 3.144) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -3.137) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 3.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -3.128) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 3.128) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -3.119) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 3.119) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -3.11) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 3.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -3.1) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -3.09) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 3.09) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -3.079) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 3.079) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -3.067) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 3.067) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -3.055) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 3.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -3.042) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 3.042) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -3.029) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 3.029) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -3.015) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 3.015) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -3.001) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 3.001) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.986) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.986) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.97) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.954) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.954) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.937) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.937) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.919) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.919) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.901) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.901) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.882) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.882) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.863) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.863) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.843) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.843) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.822) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.822) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.8) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -2.778) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 2.778) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -2.755) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 2.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -2.731) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 2.731) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -2.706) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 2.706) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -2.681) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 2.681) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -2.654) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 2.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -2.627) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 2.627) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -2.599) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 2.599) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -2.57) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 2.57) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -2.54) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -2.51) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 2.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -2.478) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 2.478) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -2.445) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 2.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -2.411) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 2.411) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -2.375) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 2.375) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -2.339) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 2.339) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -2.301) (end 3.491 2.301) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -2.262) (end 3.531 2.262) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -2.222) (end 3.571 2.222) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -2.18) (end 3.611 2.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -2.137) (end 3.651 2.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -2.092) (end 3.691 2.092) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -2.045) (end 3.731 2.045) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -1.997) (end 3.771 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -1.946) (end 3.811 1.946) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.851 -1.894) (end 3.851 1.894) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.891 -1.839) (end 3.891 1.839) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.931 -1.781) (end 3.931 1.781) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.971 -1.721) (end 3.971 1.721) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.011 -1.658) (end 4.011 1.658) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.051 -1.591) (end 4.051 1.591) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.091 -1.52) (end 4.091 1.52) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.131 -1.445) (end 4.131 1.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.171 -1.364) (end 4.171 1.364) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.211 -1.278) (end 4.211 1.278) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.251 -1.184) (end 4.251 1.184) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.291 -1.081) (end 4.291 1.081) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.331 -0.966) (end 4.331 0.966) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.371 -0.834) (end 4.371 0.834) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.411 -0.676) (end 4.411 0.676) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.451 -0.468) (end 4.451 0.468) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.25 -3.5) (end -2.25 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 3.5) (end 4.75 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 3.5) (end 4.75 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 -3.5) (end -2.25 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF) (tstamp 59ED11E0)
    (at 184.15 75.311)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (path /59D5E4BF)
    (fp_text reference Q3 (at 2.54 -3.56 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BC550C (at 2.54 2.79) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.74 1.85) (end 4.34 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 1.75) (end 4.3 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.01 -2.73) (end 6.09 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.01 -2.73) (end -1.01 2.01) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.09 2.01) (end 6.09 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.09 2.01) (end -1.01 2.01) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 2.54 0) (end 0.74 1.85) (angle 20) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.6) (angle -65) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.6) (angle 65) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.48) (angle 135) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.54 0) (end 2.54 -2.48) (angle -135) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.54 0) (end 4.34 1.85) (angle -20) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C12-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(Q3-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF) (tstamp 59ED11D9)
    (at 169.418 75.311)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (path /59D7FA67)
    (fp_text reference Q2 (at 2.54 -3.56 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BC550C (at 2.54 2.79) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.74 1.85) (end 4.34 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 1.75) (end 4.3 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.01 -2.73) (end 6.09 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.01 -2.73) (end -1.01 2.01) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.09 2.01) (end 6.09 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.09 2.01) (end -1.01 2.01) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 2.54 0) (end 0.74 1.85) (angle 20) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.6) (angle -65) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.6) (angle 65) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.48) (angle 135) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.54 0) (end 2.54 -2.48) (angle -135) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.54 0) (end 4.34 1.85) (angle -20) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(Q2-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF) (tstamp 59ED11D2)
    (at 127.508 74.803)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (path /59D5E535)
    (fp_text reference Q1 (at 2.54 -3.56 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BC550C (at 2.54 2.79) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.74 1.85) (end 4.34 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 1.75) (end 4.3 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.01 -2.73) (end 6.09 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.01 -2.73) (end -1.01 2.01) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.09 2.01) (end 6.09 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.09 2.01) (end -1.01 2.01) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 2.54 0) (end 0.74 1.85) (angle 20) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.6) (angle -65) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.6) (angle 65) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.54 0) (end 2.54 -2.48) (angle 135) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.54 0) (end 2.54 -2.48) (angle -135) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.54 0) (end 4.34 1.85) (angle -20) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module Kicad_GSM_Footprint:SolderWirePad_3x_1-2mmDrill (layer F.Cu) (tedit 59EE6176) (tstamp 5C635FFF)
    (at 74.01687 44.55287)
    (path /59DA1CC8)
    (fp_text reference J1 (at 0 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value In (at 1.27 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at -3.81 0) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 3.81 0) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask))
  )

  (module Kicad_GSM_Footprint:SolderWirePad_2x_1-2mmDrill (layer F.Cu) (tedit 59EE6AF5) (tstamp 5C636005)
    (at 82.72187 44.55287)
    (path /59DA4599)
    (fp_text reference J2 (at 0 -3.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Out (at 0.635 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at -1.905 0) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 1.905 0) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask))
  )

  (segment (start 142.875 9.779) (end 142.8496 9.8044) (width 0.25) (layer F.Cu) (net 0) (tstamp 59EE7625) (status 30))
  (segment (start 123.698 101.219) (end 123.698 107.569) (width 0.8) (layer F.Cu) (net 1))
  (segment (start 123.698 107.569) (end 123.063 108.204) (width 0.8) (layer F.Cu) (net 1) (tstamp 59F1E11B))
  (segment (start 203.835 88.519) (end 203.835 84.535) (width 0.8) (layer F.Cu) (net 2))
  (segment (start 203.835 84.535) (end 203.755 84.455) (width 0.8) (layer F.Cu) (net 2) (tstamp 59F72B8C))
  (segment (start 203.835 78.105) (end 203.835 84.375) (width 0.8) (layer F.Cu) (net 2))
  (segment (start 203.835 84.375) (end 203.755 84.455) (width 0.8) (layer F.Cu) (net 2) (tstamp 59F72B89))
  (segment (start 203.835 68.707) (end 203.835 72.517) (width 0.8) (layer F.Cu) (net 2))
  (segment (start 203.835 72.517) (end 203.835 78.105) (width 0.8) (layer F.Cu) (net 2) (tstamp 59F72B86))
  (segment (start 203.875 88.773) (end 203.835 88.733) (width 0.25) (layer F.Cu) (net 2) (tstamp 59EE79D8))
  (segment (start 206.375 83.82) (end 206.375 78.145) (width 0.8) (layer F.Cu) (net 3))
  (segment (start 206.375 78.145) (end 206.335 78.105) (width 0.8) (layer F.Cu) (net 3) (tstamp 59F72BE8))
  (segment (start 138.898 63.373) (end 150.876 63.373) (width 0.8) (layer F.Cu) (net 7))
  (segment (start 151.892 64.389) (end 151.892 65.913) (width 0.8) (layer F.Cu) (net 7) (tstamp 5A0A34F6))
  (segment (start 150.876 63.373) (end 151.892 64.389) (width 0.8) (layer F.Cu) (net 7) (tstamp 5A0A34F5))
  (segment (start 198.755 77.851) (end 198.755 76.2) (width 0.8) (layer F.Cu) (net 8))
  (segment (start 199.166002 67.152998) (end 200.406 65.913) (width 0.8) (layer F.Cu) (net 8) (tstamp 59F1D2B2))
  (segment (start 199.166002 75.788998) (end 199.166002 67.152998) (width 0.8) (layer F.Cu) (net 8) (tstamp 59F1D2AB))
  (segment (start 198.755 76.2) (end 199.166002 75.788998) (width 0.8) (layer F.Cu) (net 8) (tstamp 59F1D2A7))
  (segment (start 198.755 80.351) (end 198.755 84.455) (width 0.8) (layer F.Cu) (net 9))
  (segment (start 198.755 80.351) (end 199.811 80.351) (width 0.8) (layer F.Cu) (net 9))
  (segment (start 201.295 78.867) (end 201.295 72.517) (width 0.8) (layer F.Cu) (net 9) (tstamp 59F72BB0))
  (segment (start 199.811 80.351) (end 201.295 78.867) (width 0.8) (layer F.Cu) (net 9) (tstamp 59F72BAF))
  (segment (start 196.215 88.519) (end 196.215 86.995) (width 0.8) (layer F.Cu) (net 9))
  (segment (start 196.215 86.995) (end 198.755 84.455) (width 0.8) (layer F.Cu) (net 9) (tstamp 59F72B92))
  (segment (start 196.215 91.313) (end 196.215 88.519) (width 0.8) (layer F.Cu) (net 9))
  (segment (start 194.31 74.295) (end 194.31 71.501) (width 0.8) (layer F.Cu) (net 10))
  (segment (start 197.866 65.913) (end 197.866 75.184) (width 0.8) (layer F.Cu) (net 11))
  (segment (start 196.255 76.795) (end 194.31 76.795) (width 0.8) (layer F.Cu) (net 11) (tstamp 59F1D2A2))
  (segment (start 197.866 75.184) (end 196.255 76.795) (width 0.8) (layer F.Cu) (net 11) (tstamp 59F1D2A0))
  (segment (start 186.817 87.249) (end 186.817 91.313) (width 0.8) (layer F.Cu) (net 12))
  (segment (start 186.817 87.249) (end 188.341 87.249) (width 0.8) (layer F.Cu) (net 12))
  (segment (start 190.246 89.154) (end 191.897 89.154) (width 0.8) (layer F.Cu) (net 12) (tstamp 5A0A2718))
  (segment (start 188.341 87.249) (end 190.246 89.154) (width 0.8) (layer F.Cu) (net 12) (tstamp 5A0A2717))
  (segment (start 191.897 83.947) (end 191.897 87.154) (width 0.8) (layer F.Cu) (net 13))
  (segment (start 191.897 83.947) (end 191.897 82.63) (width 0.8) (layer F.Cu) (net 13))
  (segment (start 191.897 82.63) (end 189.277 80.01) (width 0.8) (layer F.Cu) (net 13) (tstamp 5A0A2667))
  (segment (start 186.69 75.311) (end 186.69 77.423) (width 0.8) (layer F.Cu) (net 13))
  (segment (start 186.69 77.423) (end 189.277 80.01) (width 0.8) (layer F.Cu) (net 13) (tstamp 5A0A2663))
  (segment (start 186.69 71.247) (end 186.69 75.311) (width 0.8) (layer F.Cu) (net 13))
  (segment (start 186.69 68.707) (end 186.69 71.247) (width 0.8) (layer F.Cu) (net 13))
  (segment (start 171.958 87.376) (end 171.958 91.44) (width 0.8) (layer F.Cu) (net 14))
  (segment (start 177.038 89.154) (end 175.387 89.154) (width 0.8) (layer F.Cu) (net 14))
  (segment (start 173.609 87.376) (end 171.958 87.376) (width 0.8) (layer F.Cu) (net 14) (tstamp 5A0A28CF))
  (segment (start 175.387 89.154) (end 173.609 87.376) (width 0.8) (layer F.Cu) (net 14) (tstamp 5A0A28CE))
  (segment (start 177.038 83.947) (end 177.038 87.154) (width 0.8) (layer F.Cu) (net 15))
  (segment (start 177.038 84.328) (end 177.038 82.63) (width 0.8) (layer F.Cu) (net 15))
  (segment (start 177.038 82.63) (end 174.418 80.01) (width 0.8) (layer F.Cu) (net 15) (tstamp 5A0A2613))
  (segment (start 171.958 75.311) (end 171.958 77.55) (width 0.8) (layer F.Cu) (net 15))
  (segment (start 171.958 77.55) (end 174.418 80.01) (width 0.8) (layer F.Cu) (net 15) (tstamp 5A0A260F))
  (segment (start 171.958 68.707) (end 171.958 71.247) (width 0.8) (layer F.Cu) (net 15))
  (segment (start 171.958 71.247) (end 171.958 75.311) (width 0.8) (layer F.Cu) (net 15) (tstamp 5A0A2572))
  (segment (start 189.103 61.087) (end 203.835 61.087) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 165.227 119.126) (end 166.243 120.142) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 166.243 120.142) (end 166.243 120.269) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A33E4))
  (segment (start 165.227 119.126) (end 166.243 118.11) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 166.116 118.237) (end 166.243 118.237) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A33E1))
  (segment (start 166.243 118.11) (end 166.116 118.237) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A33DF))
  (segment (start 166.243 116.713) (end 166.243 118.237) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 166.243 118.237) (end 166.243 120.269) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A33E2))
  (segment (start 166.243 120.269) (end 166.243 121.413) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A33E7))
  (segment (start 110.109 65.913) (end 110.109 108.077) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 121.158 119.126) (end 165.227 119.126) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A33D7))
  (segment (start 165.227 119.126) (end 166.243 119.126) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A33DD))
  (segment (start 110.109 108.077) (end 121.158 119.126) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A33D5))
  (segment (start 110.109 65.913) (end 110.109 62.484) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 111.506 61.087) (end 128.27 61.087) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A3268))
  (segment (start 110.109 62.484) (end 111.506 61.087) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A3267))
  (segment (start 165.481 61.087) (end 165.608 61.087) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 165.608 61.087) (end 166.37 61.849) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A2D88))
  (segment (start 167.132 61.087) (end 166.37 61.849) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A2CB1))
  (segment (start 128.27 61.087) (end 130.81 61.087) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 130.81 61.087) (end 165.481 61.087) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A2D7B))
  (segment (start 165.481 61.087) (end 171.958 61.087) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A2D86))
  (segment (start 171.958 61.087) (end 167.132 61.087) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 166.37 61.849) (end 166.37 75.057) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A2CB2))
  (segment (start 166.37 61.849) (end 167.132 61.087) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A2B52))
  (segment (start 174.498 61.087) (end 186.69 61.087) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 189.23 61.087) (end 191.77 61.087) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 186.69 61.087) (end 189.484 61.087) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 174.879 61.087) (end 184.785 61.087) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 172.2882 61.087) (end 174.879 61.087) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 206.375 61.087) (end 203.835 61.087) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 166.37 61.849) (end 167.132 61.087) (width 0.8) (layer F.Cu) (net 16) (tstamp 5A0A2A71))
  (segment (start 166.243 81.153) (end 166.243 82.677) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 166.37 61.849) (end 166.37 81.026) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 166.37 81.026) (end 166.243 81.153) (width 0.8) (layer F.Cu) (net 16))
  (segment (start 147.622999 89.966999) (end 149.223 91.567) (width 0.8) (layer F.Cu) (net 17))
  (segment (start 147.622999 85.699001) (end 147.622999 89.966999) (width 0.8) (layer F.Cu) (net 17))
  (segment (start 161.243 75.184) (end 158.138 75.184) (width 0.8) (layer F.Cu) (net 17))
  (segment (start 158.138 75.184) (end 147.622999 85.699001) (width 0.8) (layer F.Cu) (net 17))
  (segment (start 160.430001 83.489999) (end 161.243 82.677) (width 0.8) (layer F.Cu) (net 18))
  (segment (start 149.223 86.567) (end 152.300001 83.489999) (width 0.8) (layer F.Cu) (net 18))
  (segment (start 152.300001 83.489999) (end 160.430001 83.489999) (width 0.8) (layer F.Cu) (net 18))
  (segment (start 134.112 93.98) (end 134.112 91.313) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 134.112 91.313) (end 136.144 89.281) (width 0.8) (layer F.Cu) (net 19) (tstamp 5A0A31AB))
  (segment (start 134.248001 85.344) (end 134.502001 87.639001) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 134.248001 70.983999) (end 134.248001 85.344) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 136.206001 69.025999) (end 134.248001 70.983999) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 134.502001 87.639001) (end 136.144 89.281) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 158.623 68.326) (end 157.923001 69.025999) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 149.352 65.913) (end 149.352 66.99063) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 149.352 68.136999) (end 150.241 69.025999) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 157.923001 69.025999) (end 150.241 69.025999) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 149.352 68.072) (end 149.352 69.025999) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 150.241 69.025999) (end 149.352 69.025999) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 149.352 66.99063) (end 149.352 68.072) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 149.352 68.136999) (end 148.463 69.025999) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 149.352 68.072) (end 149.352 68.136999) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 149.352 69.025999) (end 148.463 69.025999) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 148.463 69.025999) (end 136.206001 69.025999) (width 0.8) (layer F.Cu) (net 19))
  (segment (start 139.502 93.59) (end 139.112 93.98) (width 0.8) (layer F.Cu) (net 20) (tstamp 5A0A31A5))
  (segment (start 145.923 93.067) (end 145.923 91.567) (width 0.8) (layer F.Cu) (net 20))
  (segment (start 145.01 93.98) (end 145.923 93.067) (width 0.8) (layer F.Cu) (net 20))
  (segment (start 139.112 93.98) (end 145.01 93.98) (width 0.8) (layer F.Cu) (net 20))
  (segment (start 143.637 84.281) (end 145.923 86.567) (width 0.8) (layer F.Cu) (net 21))
  (segment (start 136.144 84.281) (end 143.637 84.281) (width 0.8) (layer F.Cu) (net 21))
  (segment (start 157.099 92.71) (end 158.75 92.71) (width 0.8) (layer F.Cu) (net 22))
  (segment (start 164.211 89.662) (end 166.497 87.376) (width 0.8) (layer F.Cu) (net 22) (tstamp 5A0A3484))
  (segment (start 161.798 89.662) (end 164.211 89.662) (width 0.8) (layer F.Cu) (net 22) (tstamp 5A0A3483))
  (segment (start 158.75 92.71) (end 161.798 89.662) (width 0.8) (layer F.Cu) (net 22) (tstamp 5A0A3482))
  (segment (start 169.418 87.376) (end 166.497 87.376) (width 0.8) (layer F.Cu) (net 22))
  (segment (start 169.418 87.376) (end 169.418 91.44) (width 0.8) (layer F.Cu) (net 22))
  (segment (start 169.418 83.947) (end 169.418 87.376) (width 0.8) (layer F.Cu) (net 22))
  (segment (start 169.418 80.01) (end 169.418 83.947) (width 0.8) (layer F.Cu) (net 22))
  (segment (start 169.418 75.311) (end 169.418 80.01) (width 0.8) (layer F.Cu) (net 22))
  (segment (start 178.435 80.097) (end 184.19 80.097) (width 0.8) (layer F.Cu) (net 23))
  (segment (start 184.19 80.097) (end 184.277 80.01) (width 0.8) (layer F.Cu) (net 23) (tstamp 5A0A3580))
  (segment (start 184.277 87.249) (end 181.356 87.249) (width 0.8) (layer F.Cu) (net 23))
  (segment (start 184.237 79.97) (end 184.277 80.01) (width 0.8) (layer F.Cu) (net 23) (tstamp 5A0A2753))
  (segment (start 184.277 91.313) (end 184.277 87.249) (width 0.8) (layer F.Cu) (net 23))
  (segment (start 184.277 87.249) (end 184.277 83.947) (width 0.8) (layer F.Cu) (net 23) (tstamp 5A0A271D))
  (segment (start 184.277 80.391) (end 184.277 84.328) (width 0.8) (layer F.Cu) (net 23))
  (segment (start 184.15 75.311) (end 184.15 76.835) (width 0.8) (layer F.Cu) (net 23))
  (segment (start 184.15 76.835) (end 184.15 77.978) (width 0.8) (layer F.Cu) (net 23) (tstamp 5A0A25FF))
  (segment (start 184.15 77.978) (end 184.15 79.121) (width 0.8) (layer F.Cu) (net 23) (tstamp 5A0A25FD))
  (segment (start 184.15 79.121) (end 184.15 80.264) (width 0.8) (layer F.Cu) (net 23) (tstamp 5A0A2609))
  (segment (start 184.15 80.264) (end 184.277 80.391) (width 0.8) (layer F.Cu) (net 23) (tstamp 5A0A25F2))
  (segment (start 178.435 77.597) (end 178.435 72.39) (width 0.8) (layer F.Cu) (net 24) (status 10))
  (segment (start 178.435 72.39) (end 179.578 71.247) (width 0.8) (layer F.Cu) (net 24) (tstamp 5A0A2756))
  (segment (start 123.063 88.9762) (end 123.0884 88.9508) (width 0.25) (layer F.Cu) (net 25) (tstamp 59EE761C))
  (segment (start 130.048 85.979) (end 127.508 85.979) (width 0.8) (layer F.Cu) (net 25))
  (segment (start 127.508 85.979) (end 127.508 88.773) (width 0.8) (layer F.Cu) (net 25))
  (segment (start 181.356 94.996) (end 200.152 94.996) (width 0.8) (layer F.Cu) (net 25))
  (segment (start 200.152 94.996) (end 203.835 91.313) (width 0.8) (layer F.Cu) (net 25) (tstamp 5A0A34A7))
  (segment (start 116.713 88.773) (end 125.73 88.773) (width 0.8) (layer F.Cu) (net 25))
  (segment (start 166.497 98.171) (end 157.734 98.171) (width 0.8) (layer F.Cu) (net 25))
  (segment (start 157.734 98.171) (end 154.813 101.092) (width 0.8) (layer F.Cu) (net 25) (tstamp 5A0A3012))
  (segment (start 166.497 94.996) (end 166.497 98.171) (width 0.8) (layer F.Cu) (net 25))
  (segment (start 166.497 94.996) (end 181.356 94.996) (width 0.8) (layer F.Cu) (net 25))
  (segment (start 130.683 108.204) (end 130.683 104.394) (width 0.8) (layer F.Cu) (net 26))
  (segment (start 130.683 104.394) (end 127.508 101.219) (width 0.8) (layer F.Cu) (net 26) (tstamp 59F1E121))
  (segment (start 127.508 91.313) (end 119.173 91.313) (width 0.8) (layer F.Cu) (net 26))
  (segment (start 119.173 91.313) (end 116.713 93.773) (width 0.8) (layer F.Cu) (net 26) (tstamp 59F1E111))
  (segment (start 127.508 91.313) (end 127.508 101.219) (width 0.8) (layer F.Cu) (net 26))
  (segment (start 116.76 93.726) (end 116.713 93.773) (width 0.8) (layer F.Cu) (net 26) (tstamp 5A0A324D))
  (segment (start 165.1 103.378) (end 165.1 110.87) (width 0.8) (layer F.Cu) (net 27))
  (segment (start 165.1 110.87) (end 166.243 112.013) (width 0.8) (layer F.Cu) (net 27) (tstamp 5A0A33B9))
  (segment (start 174.117 98.171) (end 174.117 101.727) (width 0.8) (layer F.Cu) (net 28))
  (segment (start 172.466 103.378) (end 167.64 103.378) (width 0.8) (layer F.Cu) (net 28) (tstamp 5A0A33B6))
  (segment (start 174.117 101.727) (end 172.466 103.378) (width 0.8) (layer F.Cu) (net 28) (tstamp 5A0A33B5))
  (segment (start 174.498 68.707) (end 174.498 75.311) (width 0.8) (layer F.Cu) (net 30))
  (segment (start 189.23 68.707) (end 189.23 75.311) (width 0.8) (layer F.Cu) (net 31))
  (segment (start 206.375 72.517) (end 206.375 68.707) (width 0.8) (layer F.Cu) (net 32))
  (segment (start 160.943 121.413) (end 160.943 123.097) (width 0.8) (layer F.Cu) (net 40))
  (segment (start 171.543 123.224) (end 171.543 121.413) (width 0.8) (layer F.Cu) (net 40) (tstamp 5A0A33EC))
  (segment (start 170.434 124.333) (end 171.543 123.224) (width 0.8) (layer F.Cu) (net 40) (tstamp 5A0A33EB))
  (segment (start 162.179 124.333) (end 170.434 124.333) (width 0.8) (layer F.Cu) (net 40) (tstamp 5A0A33EA))
  (segment (start 160.943 123.097) (end 162.179 124.333) (width 0.8) (layer F.Cu) (net 40) (tstamp 5A0A33E9))
  (segment (start 195.326 65.913) (end 194.564 65.913) (width 0.8) (layer F.Cu) (net 33))
  (segment (start 194.564 65.913) (end 191.77 68.707) (width 0.8) (layer F.Cu) (net 33) (tstamp 59F1D29D))
  (segment (start 126.873 108.204) (end 126.873 110.363) (width 0.8) (layer F.Cu) (net 34))
  (segment (start 134.493 110.49) (end 134.493 101.092) (width 0.8) (layer F.Cu) (net 34) (tstamp 5A0A352D))
  (segment (start 133.096 111.887) (end 134.493 110.49) (width 0.8) (layer F.Cu) (net 34) (tstamp 5A0A352C))
  (segment (start 128.397 111.887) (end 133.096 111.887) (width 0.8) (layer F.Cu) (net 34) (tstamp 5A0A352B))
  (segment (start 126.873 110.363) (end 128.397 111.887) (width 0.8) (layer F.Cu) (net 34) (tstamp 5A0A352A))
  (segment (start 153.122 89.067) (end 149.223 89.067) (width 0.8) (layer F.Cu) (net 35))
  (segment (start 157.099 85.09) (end 153.122 89.067) (width 0.8) (layer F.Cu) (net 35))
  (segment (start 162.687 85.09) (end 157.099 85.09) (width 0.8) (layer F.Cu) (net 35))
  (segment (start 163.83 67.945) (end 163.957 83.82) (width 0.8) (layer F.Cu) (net 35))
  (segment (start 154.432 65.913) (end 161.798 65.913) (width 0.8) (layer F.Cu) (net 35))
  (segment (start 163.957 83.82) (end 162.687 85.09) (width 0.8) (layer F.Cu) (net 35))
  (segment (start 161.798 65.913) (end 163.83 67.945) (width 0.8) (layer F.Cu) (net 35))
  (segment (start 171.543 112.013) (end 199.264 112.013) (width 0.8) (layer F.Cu) (net 36))
  (segment (start 206.375 104.902) (end 206.375 91.44) (width 0.8) (layer F.Cu) (net 36) (tstamp 5A0A33C5))
  (segment (start 199.264 112.013) (end 206.375 104.902) (width 0.8) (layer F.Cu) (net 36) (tstamp 5A0A33C3))
  (segment (start 160.943 112.013) (end 160.943 112.488) (width 0.8) (layer F.Cu) (net 38))
  (segment (start 160.943 112.488) (end 159.131 114.3) (width 0.8) (layer F.Cu) (net 38) (tstamp 5A0A3418))
  (segment (start 159.131 114.3) (end 119.888 114.3) (width 0.8) (layer F.Cu) (net 38) (tstamp 5A0A3419))
  (segment (start 119.888 114.3) (end 112.649 107.061) (width 0.8) (layer F.Cu) (net 38) (tstamp 5A0A341A))
  (segment (start 112.649 107.061) (end 112.649 65.913) (width 0.8) (layer F.Cu) (net 38) (tstamp 5A0A341C))

)
