From 3338bcb05479f1149420d4a0ea3904cb9e42eef5 Mon Sep 17 00:00:00 2001
From: Jean-Christophe PLAGNIOL-VILLARD <plagnioj@jcrosoft.com>
Date: Wed, 14 Nov 2012 19:18:22 +0800
Subject: [PATCH 3/5] at91sam9260/9g20: add wathdog support

Signed-off-by: Jean-Christophe PLAGNIOL-VILLARD <plagnioj@jcrosoft.com>
---
 arch/arm/mach-at91/at91sam9260_devices.c | 12 ++++++++++++
 1 file changed, 12 insertions(+)

diff --git a/arch/arm/mach-at91/at91sam9260_devices.c b/arch/arm/mach-at91/at91sam9260_devices.c
index 1c375ee..5885f91 100644
--- a/arch/arm/mach-at91/at91sam9260_devices.c
+++ b/arch/arm/mach-at91/at91sam9260_devices.c
@@ -10,6 +10,7 @@
  *
  */
 #include <common.h>
+#include <init.h>
 #include <sizes.h>
 #include <asm/armlinux.h>
 #include <asm/hardware.h>
@@ -397,3 +398,14 @@ void at91_add_device_mci(short mmc_id, struct atmel_mci_platform_data *data)
 #else
 void at91_add_device_mci(short mmc_id, struct atmel_mci_platform_data *data) {}
 #endif
+
+#ifdef CONFIG_WATCHDOG_AT91SAM9X
+static int at91_add_device_watchdog(void)
+{
+	add_generic_device("at91sam9_wdt", DEVICE_ID_SINGLE, NULL,
+		AT91_WDT + AT91_BASE_SYS, 16, IORESOURCE_MEM, NULL);
+
+	return 0;
+}
+coredevice_initcall(at91_add_device_watchdog);
+#endif
-- 
1.8.1.4

