#
# \brief  Test for the TCP terminal
# \author Norman Feske
# \date   2011-09-08
#

#
# TODO: Add support for Linux via user-level networking (using the
#       tun/tap proxy driver at os/src/drivers/nic/linux)
#
if {[have_spec linux]} {
	puts "Run script does not support Linux."; exit 0 }

#
# Build
#

set build_components {
	core init
	drivers/timer drivers/nic
	server/tcp_terminal
	test/terminal_echo
}

source ${genode_dir}/repos/base/run/platform_drv.inc
append_platform_drv_build_components

build $build_components

create_boot_directory

#
# Generate config
#

set config {
<config verbose="yes">
	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<default caps="100"/>
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Timer"/> </provides>
	</start>
	<start name="nic_drv">
		<resource name="RAM" quantum="4M"/>
		<provides> <service name="Nic"/> </provides>
	</start>
	<start name="tcp_terminal" caps="200">
		<resource name="RAM" quantum="2560K"/>
		<provides> <service name="Terminal"/> </provides>
		<config>
			<policy label_prefix="test-terminal_echo" port="8888"/>
			<vfs> <dir name="dev"> <log/> </dir> </vfs>
			<libc stdout="/dev/log"/>
		</config>
	</start>
	<start name="test-terminal_echo">
		<resource name="RAM" quantum="1M"/>
	</start>}

append_platform_drv_config

append config {
</config>
}

install_config $config

#
# Boot modules
#

# generic modules
set boot_modules {
	core ld.lib.so init timer
	nic_drv
	libc.lib.so pthread.lib.so lwip.lib.so libc_pipe.lib.so
	tcp_terminal
	test-terminal_echo
}

# platform-specific modules
append_platform_drv_boot_modules

build_boot_image $boot_modules

#
# Execute test
#

# qemu config
append qemu_args "  -nographic "

append_if [have_spec x86]     qemu_args " -net nic,model=e1000 "
append_if [have_spec lan9118] qemu_args " -net nic,model=lan9118 "

append qemu_args " -net user -redir tcp:5555::8888 "

run_genode_until forever

#
# Now, connect via 'telnet localhost 5555'
#

# vi: set ft=tcl :
