(export (version D)
  (design
    (source "/home/eri/netzBiotop e.V./tuer/Fuzzzy.sch")
    (date "Tue 24 Oct 2017 12:20:22 AM CEST")
    (tool "Eeschema 4.0.7+dfsg1-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Fuzzzy.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref Q4)
      (value BC550C)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib transistors) (part BC237))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D5E492))
    (comp (ref Q3)
      (value BC550C)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib transistors) (part BC237))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D5E4BF))
    (comp (ref Q1)
      (value BC550C)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib transistors) (part BC237))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D5E535))
    (comp (ref R13)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7B711))
    (comp (ref C10)
      (value 470pF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7B9C6))
    (comp (ref R9)
      (value 470k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7BB68))
    (comp (ref R14)
      (value 47k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7BC56))
    (comp (ref C1)
      (value 10µF)
      (footprint Capacitors_THT:CP_Radial_D6.3mm_P2.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7BD49))
    (comp (ref R2)
      (value 33k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7BFBD))
    (comp (ref R22)
      (value 120)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7C852))
    (comp (ref C4)
      (value 0.1µF)
      (footprint Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02)
      (fields
        (field (name Type) "Wima MKS"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7C93F))
    (comp (ref R24)
      (value 100k)
      (footprint Kicad_GSM_Footprint:POT)
      (datasheet Sustain)
      (fields
        (field (name Type) linear))
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7C9EC))
    (comp (ref R23)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7CA93))
    (comp (ref C5)
      (value 0.1µF)
      (footprint Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02)
      (fields
        (field (name Type) "Wima MKS"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7CC75))
    (comp (ref R19)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7CD55))
    (comp (ref R17)
      (value 470k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7D143))
    (comp (ref C12)
      (value 470pF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7D1E6))
    (comp (ref C6)
      (value 1µF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.00mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7D2A1))
    (comp (ref D3)
      (value 1N914)
      (footprint Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7D7EC))
    (comp (ref D4)
      (value 1N914)
      (footprint Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_KathodeUp)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7D8BD))
    (comp (ref R18)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7DEF4))
    (comp (ref R20)
      (value 100k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7E4FA))
    (comp (ref R21)
      (value 150k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7E756))
    (comp (ref Q2)
      (value BC550C)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib transistors) (part BC237))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA67))
    (comp (ref C13)
      (value 0.1µF)
      (footprint Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02)
      (fields
        (field (name Type) "Wima MKS"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA6E))
    (comp (ref R12)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA75))
    (comp (ref R15)
      (value 470k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA7C))
    (comp (ref C11)
      (value 470pF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA83))
    (comp (ref D1)
      (value 1N914)
      (footprint Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA91))
    (comp (ref D2)
      (value 1N914)
      (footprint Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_KathodeUp)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA98))
    (comp (ref R11)
      (value 15k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA9F))
    (comp (ref R16)
      (value 100k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FAAC))
    (comp (ref R10)
      (value 150k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FAB3))
    (comp (ref C7)
      (value 1µF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.00mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA8A))
    (comp (ref R8)
      (value 33k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D863A5))
    (comp (ref R25)
      (value 100k)
      (footprint Kicad_GSM_Footprint:POT)
      (fields
        (field (name Type) Linear))
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D866C7))
    (comp (ref C8a1)
      (value 0.01µF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D87D85))
    (comp (ref C8b1)
      (value 0.0056µF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D8860E))
    (comp (ref C9a1)
      (value 0.004µF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D8CA79))
    (comp (ref C9b1)
      (value 0.01µF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D8CDB4))
    (comp (ref R5)
      (value 22k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D8E71F))
    (comp (ref C3)
      (value 0.1µF)
      (footprint Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02)
      (fields
        (field (name Type) "Wima MKS"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D90B52))
    (comp (ref R7)
      (value 430k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D91739))
    (comp (ref R3)
      (value 100k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D91E8D))
    (comp (ref R4)
      (value 3k3)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D92708))
    (comp (ref R6)
      (value 15k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D92E3C))
    (comp (ref C2)
      (value 1µF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.00mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D937BB))
    (comp (ref R26)
      (value 100k)
      (footprint Kicad_GSM_Footprint:POT)
      (fields
        (field (name Type) Log))
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D9398C))
    (comp (ref J1)
      (value In)
      (footprint Wire_Pads:SolderWirePad_3x_1-2mmDrill)
      (libsource (lib conn) (part Audio-Jack-3))
      (sheetpath (names /) (tstamps /))
      (tstamp 59DA1CC8))
    (comp (ref J2)
      (value Out)
      (footprint Wire_Pads:SolderWirePad_2x_1mmDrill)
      (libsource (lib conn) (part Audio-Jack-2))
      (sheetpath (names /) (tstamps /))
      (tstamp 59DA4599))
    (comp (ref J3)
      (value Jack-DC)
      (footprint Kicad_GSM_Footprint:SolderWirePad_3x_1-2mmDrill)
      (libsource (lib conn) (part Jack-DC))
      (sheetpath (names /) (tstamps /))
      (tstamp 59E13C16))
    (comp (ref BT1)
      (value 9V)
      (footprint Kicad_GSM_Footprint:SolderWirePad_2x_1-2mmDrill_numbered)
      (libsource (lib device) (part Battery_Cell))
      (sheetpath (names /) (tstamps /))
      (tstamp 59E1758A))
    (comp (ref D5)
      (value 1N4001)
      (footprint Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 59E92029))
    (comp (ref C14)
      (value 470µF)
      (footprint Capacitors_THT:CP_Radial_D13.0mm_P5.00mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 59E9510F))
    (comp (ref R27)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0617_L17.0mm_D6.0mm_P20.32mm_Horizontal)
      (fields
        (field (name Type) 5W))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59EA3323))
    (comp (ref Q5)
      (value SW-3PDT)
      (footprint Kicad_GSM_Footprint:3PDT)
      (libsource (lib Fuzzzy-cache) (part SW-3PDT))
      (sheetpath (names /) (tstamps /))
      (tstamp 59EA702A))
    (comp (ref D6)
      (value "LED 1.8V")
      (footprint LEDs:LED_D5.0mm)
      (fields
        (field (name Type) "low current orange 1.8V"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 59EB5D9D))
    (comp (ref R28)
      (value 3.3k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59EB7B94))
    (comp (ref Q6)
      (value SW-DPDT)
      (footprint Kicad_GSM_Footprint:DPDT)
      (libsource (lib Fuzzzy-cache) (part SW-DPDT))
      (sheetpath (names /) (tstamps /))
      (tstamp 59EE6A68)))
  (libparts
    (libpart (lib conn) (part Audio-Jack-2)
      (description "2-pin audio jack receptable (mono/TS connector)")
      (docs ~)
      (fields
        (field (name Reference) J)
        (field (name Value) Audio-Jack-2))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Audio-Jack-3)
      (description "3-pin audio jack receptable (stereo/TRS connector)")
      (docs ~)
      (fields
        (field (name Reference) J)
        (field (name Value) Audio-Jack-3))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib transistors) (part BC237)
      (description "Vce 50V, Ic 100mA, NPN Epitaxial Silicon Transistor, TO-92")
      (docs http://www.onsemi.com/pub_link/Collateral/BC237-D.PDF)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BC237)
        (field (name Footprint) TO_SOT_Packages_THT:TO-92_Molded_Narrow))
      (pins
        (pin (num 1) (name C) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name E) (type passive))))
    (libpart (lib conn) (part Barrel_Jack)
      (aliases
        (alias Jack-DC))
      (description "DC Barrel Jack")
      (docs ~)
      (fields
        (field (name Reference) J)
        (field (name Value) Barrel_Jack))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib device) (part Battery_Cell)
      (description "single battery cell")
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part D)
      (description Diode)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part LED)
      (description "LED generic")
      (footprints
        (fp LED*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part POT)
      (description Potentiometer)
      (footprints
        (fp Potentiometer*))
      (fields
        (field (name Reference) RV)
        (field (name Value) POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Fuzzzy-cache) (part SW-3PDT)
      (fields
        (field (name Reference) Q)
        (field (name Value) SW-3PDT))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type input))
        (pin (num 7) (name ~) (type input))
        (pin (num 8) (name ~) (type input))
        (pin (num 9) (name ~) (type input))))
    (libpart (lib Fuzzzy-cache) (part SW-DPDT)
      (fields
        (field (name Reference) Q)
        (field (name Value) SW-DPDT))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type input)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical transistors)
      (uri /usr/share/kicad/library/transistors.lib))
    (library (logical Fuzzzy-cache)
      (uri "/home/eri/netzBiotop e.V./tuer/Fuzzzy-cache.lib")))
  (nets
    (net (code 1) (name "Net-(C6-Pad1)")
      (node (ref D3) (pin 1))
      (node (ref D4) (pin 2))
      (node (ref C6) (pin 1)))
    (net (code 2) (name "Net-(C7-Pad1)")
      (node (ref D2) (pin 2))
      (node (ref D1) (pin 1))
      (node (ref C7) (pin 1)))
    (net (code 3) (name "Net-(Q2-Pad3)")
      (node (ref Q2) (pin 3))
      (node (ref R10) (pin 1)))
    (net (code 4) (name "Net-(C2-Pad1)")
      (node (ref Q1) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref C2) (pin 1)))
    (net (code 5) (name "Net-(Q1-Pad3)")
      (node (ref Q1) (pin 3))
      (node (ref R4) (pin 1)))
    (net (code 6) (name "Net-(C3-Pad1)")
      (node (ref C3) (pin 1))
      (node (ref R7) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref R3) (pin 1)))
    (net (code 7) (name "Net-(C9a1-Pad1)")
      (node (ref C9b1) (pin 1))
      (node (ref R25) (pin 1))
      (node (ref R5) (pin 2))
      (node (ref C9a1) (pin 1)))
    (net (code 8) (name "Net-(Q3-Pad3)")
      (node (ref Q3) (pin 3))
      (node (ref R21) (pin 1)))
    (net (code 9) (name "Net-(C12-Pad2)")
      (node (ref R19) (pin 1))
      (node (ref R20) (pin 1))
      (node (ref R17) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref Q3) (pin 2)))
    (net (code 10) (name "Net-(C2-Pad2)")
      (node (ref R26) (pin 1))
      (node (ref C2) (pin 2)))
    (net (code 11) (name "Net-(C11-Pad2)")
      (node (ref R16) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref Q2) (pin 2)))
    (net (code 12) (name "Net-(C13-Pad1)")
      (node (ref C13) (pin 1))
      (node (ref R12) (pin 2)))
    (net (code 13) (name "Net-(C12-Pad1)")
      (node (ref D4) (pin 1))
      (node (ref R17) (pin 1))
      (node (ref C13) (pin 2))
      (node (ref C12) (pin 1))
      (node (ref Q3) (pin 1))
      (node (ref D3) (pin 2))
      (node (ref R18) (pin 2)))
    (net (code 14) (name "Net-(C9b1-Pad2)")
      (node (ref Q6) (pin 6))
      (node (ref C9b1) (pin 2)))
    (net (code 15) (name "Net-(C11-Pad1)")
      (node (ref Q6) (pin 5))
      (node (ref R8) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref Q2) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref R11) (pin 2)))
    (net (code 16) (name "Net-(C9a1-Pad2)")
      (node (ref C9a1) (pin 2))
      (node (ref Q6) (pin 4)))
    (net (code 17) (name "Net-(C8a1-Pad2)")
      (node (ref C8a1) (pin 2))
      (node (ref Q6) (pin 3)))
    (net (code 18) (name "Net-(C8b1-Pad2)")
      (node (ref C8b1) (pin 2))
      (node (ref Q6) (pin 1)))
    (net (code 19) (name "Net-(J3-Pad2)")
      (node (ref R27) (pin 2))
      (node (ref J3) (pin 2)))
    (net (code 20) (name "Net-(BT1-Pad1)")
      (node (ref J3) (pin 3))
      (node (ref BT1) (pin 1)))
    (net (code 21) (name Earth)
      (node (ref R20) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref R5) (pin 1))
      (node (ref R23) (pin 2))
      (node (ref R22) (pin 2))
      (node (ref Q5) (pin 6))
      (node (ref Q5) (pin 5))
      (node (ref C8b1) (pin 1))
      (node (ref R3) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref R26) (pin 3))
      (node (ref R16) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref J1) (pin 3))
      (node (ref C8a1) (pin 1)))
    (net (code 22) (name "Net-(Q5-Pad7)")
      (node (ref Q5) (pin 7))
      (node (ref R2) (pin 2)))
    (net (code 23) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref Q5) (pin 8)))
    (net (code 24) (name "Net-(Q6-Pad2)")
      (node (ref R25) (pin 3))
      (node (ref R8) (pin 2))
      (node (ref Q6) (pin 2)))
    (net (code 25) (name "Net-(BT1-Pad2)")
      (node (ref C14) (pin 2))
      (node (ref D5) (pin 2))
      (node (ref BT1) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref J3) (pin 1)))
    (net (code 26) (name "Net-(D6-Pad2)")
      (node (ref R28) (pin 2))
      (node (ref D6) (pin 2)))
    (net (code 27) (name "Net-(D6-Pad1)")
      (node (ref Q5) (pin 4))
      (node (ref D6) (pin 1)))
    (net (code 28) (name +9V)
      (node (ref R7) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref R27) (pin 1))
      (node (ref D5) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref R13) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref R28) (pin 1)))
    (net (code 29) (name "Net-(Q5-Pad1)")
      (node (ref Q5) (pin 1))
      (node (ref R26) (pin 2)))
    (net (code 30) (name "Net-(J2-Pad1)")
      (node (ref J2) (pin 1))
      (node (ref Q5) (pin 2)))
    (net (code 31) (name "Net-(Q5-Pad3)")
      (node (ref Q5) (pin 3))
      (node (ref Q5) (pin 9)))
    (net (code 32) (name "Net-(C3-Pad2)")
      (node (ref R25) (pin 2))
      (node (ref C3) (pin 2)))
    (net (code 33) (name "Net-(C1-Pad2)")
      (node (ref C1) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 34) (name "Net-(Q4-Pad3)")
      (node (ref R22) (pin 1))
      (node (ref Q4) (pin 3)))
    (net (code 35) (name "Net-(C5-Pad2)")
      (node (ref R24) (pin 2))
      (node (ref C5) (pin 2)))
    (net (code 36) (name "Net-(C5-Pad1)")
      (node (ref C5) (pin 1))
      (node (ref R19) (pin 2)))
    (net (code 37) (name "Net-(R23-Pad1)")
      (node (ref R24) (pin 3))
      (node (ref R23) (pin 1)))
    (net (code 38) (name "Net-(C4-Pad1)")
      (node (ref C4) (pin 1))
      (node (ref R24) (pin 1)))
    (net (code 39) (name "Net-(C1-Pad1)")
      (node (ref Q4) (pin 2))
      (node (ref C1) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref R9) (pin 2))
      (node (ref C10) (pin 2)))
    (net (code 40) (name "Net-(C10-Pad1)")
      (node (ref Q4) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref R9) (pin 1)))))