(export (version D)
  (design
    (source /home/eri/projects/git-repos/Deffekt/Deffekt.sch)
    (date "Wed 13 Feb 2019 01:14:13 AM CET")
    (tool "Eeschema 5.0.2+dfsg1-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Deffekt.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref Q4)
      (value BC550C)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib Transistor_BJT) (part BC550) (description "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D5E492))
    (comp (ref Q3)
      (value BC550C)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib Transistor_BJT) (part BC550) (description "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D5E4BF))
    (comp (ref Q1)
      (value BC550C)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib Transistor_BJT) (part BC550) (description "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D5E535))
    (comp (ref R13)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7B711))
    (comp (ref C10)
      (value 470pF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7B9C6))
    (comp (ref R9)
      (value 470k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7BB68))
    (comp (ref R14)
      (value 47k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7BC56))
    (comp (ref C1)
      (value 10µF)
      (footprint Capacitors_THT:CP_Radial_D6.3mm_P2.50mm)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7BD49))
    (comp (ref R2)
      (value 33k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7BFBD))
    (comp (ref R22)
      (value 120)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7C852))
    (comp (ref C4)
      (value 0.1µF)
      (footprint Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02)
      (fields
        (field (name Type) "Wima MKS"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7C93F))
    (comp (ref R24)
      (value 100k)
      (footprint Kicad_GSM_Footprint:POT)
      (datasheet Sustain)
      (fields
        (field (name Type) linear))
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7C9EC))
    (comp (ref R23)
      (value 1k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7CA93))
    (comp (ref C5)
      (value 0.1µF)
      (footprint Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02)
      (fields
        (field (name Type) "Wima MKS"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7CC75))
    (comp (ref R19)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7CD55))
    (comp (ref R17)
      (value 470k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7D143))
    (comp (ref C12)
      (value 470pF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7D1E6))
    (comp (ref C6)
      (value 1µF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.00mm)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7D2A1))
    (comp (ref D3)
      (value 1N914)
      (footprint Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7D7EC))
    (comp (ref D4)
      (value 1N914)
      (footprint Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_KathodeUp)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7D8BD))
    (comp (ref R18)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7DEF4))
    (comp (ref R20)
      (value 100k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7E4FA))
    (comp (ref R21)
      (value 150k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7E756))
    (comp (ref Q2)
      (value BC550C)
      (footprint TO_SOT_Packages_THT:TO-92_Molded_Narrow)
      (libsource (lib Transistor_BJT) (part BC550) (description "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA67))
    (comp (ref C13)
      (value 0.1µF)
      (footprint Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02)
      (fields
        (field (name Type) "Wima MKS"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA6E))
    (comp (ref R12)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA75))
    (comp (ref R15)
      (value 470k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA7C))
    (comp (ref C11)
      (value 470pF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA83))
    (comp (ref D1)
      (value 1N914)
      (footprint Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA91))
    (comp (ref D2)
      (value 1N914)
      (footprint Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_KathodeUp)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA98))
    (comp (ref R11)
      (value 15k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA9F))
    (comp (ref R16)
      (value 100k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FAAC))
    (comp (ref R10)
      (value 150k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FAB3))
    (comp (ref C7)
      (value 1µF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.00mm)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D7FA8A))
    (comp (ref R8)
      (value 33k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D863A5))
    (comp (ref R25)
      (value 100k)
      (footprint Kicad_GSM_Footprint:POT)
      (fields
        (field (name Type) Linear))
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D866C7))
    (comp (ref C8a1)
      (value 0.01µF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D87D85))
    (comp (ref C8b1)
      (value 0.0056µF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D8860E))
    (comp (ref C9a1)
      (value 0.004µF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D8CA79))
    (comp (ref C9b1)
      (value 0.01µF)
      (footprint Capacitors_THT:C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2)
      (fields
        (field (name Type) "Wima FKP2"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D8CDB4))
    (comp (ref R5)
      (value 22k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D8E71F))
    (comp (ref C3)
      (value 0.1µF)
      (footprint Capacitors_THT:C_Rect_L4.6mm_W2.5mm_P2.50mm_MKS02_FKP02)
      (fields
        (field (name Type) "Wima MKS"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D90B52))
    (comp (ref R7)
      (value 430k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D91739))
    (comp (ref R3)
      (value 100k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D91E8D))
    (comp (ref R4)
      (value 3k3)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D92708))
    (comp (ref R6)
      (value 15k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D92E3C))
    (comp (ref C2)
      (value 1µF)
      (footprint Capacitors_THT:CP_Radial_D5.0mm_P2.00mm)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D937BB))
    (comp (ref R26)
      (value 100k)
      (footprint Kicad_GSM_Footprint:POT)
      (fields
        (field (name Type) Log))
      (libsource (lib Device) (part R_POT) (description Potentiometer))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D9398C))
    (comp (ref J1)
      (value In)
      (footprint Kicad_GSM_Footprint:SolderWirePad_3x_1-2mmDrill)
      (libsource (lib Connector) (part AudioJack3_Ground) (description "Audio Jack, 3 Poles (Stereo / TRS), Grounded Sleeve"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59DA1CC8))
    (comp (ref J2)
      (value Out)
      (footprint Kicad_GSM_Footprint:SolderWirePad_2x_1-2mmDrill)
      (libsource (lib Connector) (part AudioJack2_Ground) (description "Audio Jack, 2 Poles (Mono / TS), Grounded Sleeve"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59DA4599))
    (comp (ref J3)
      (value Jack-DC)
      (footprint Kicad_GSM_Footprint:SolderWirePad_3x_1-2mmDrill)
      (libsource (lib Connector) (part Barrel_Jack_Switch) (description "DC Barrel Jack with an internal switch"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59E13C16))
    (comp (ref BT1)
      (value 9V)
      (footprint Kicad_GSM_Footprint:SolderWirePad_2x_1-2mmDrill_numbered)
      (libsource (lib Device) (part Battery_Cell) (description "Single-cell battery"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59E1758A))
    (comp (ref D5)
      (value 1N4001)
      (footprint Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp)
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 59E92029))
    (comp (ref C14)
      (value 470µF)
      (footprint Capacitors_THT:CP_Radial_D13.0mm_P5.00mm)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59E9510F))
    (comp (ref R27)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0617_L17.0mm_D6.0mm_P20.32mm_Horizontal)
      (fields
        (field (name Type) 5W))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59EA3323))
    (comp (ref D6)
      (value "LED 1.8V")
      (footprint LEDs:LED_D5.0mm)
      (fields
        (field (name Type) "low current orange 1.8V"))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59EB5D9D))
    (comp (ref R28)
      (value 3.3k)
      (footprint Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 59EB7B94))
    (comp (ref S1)
      (value SWITCH-3PDT)
      (footprint Kicad_GSM_Footprint:3PDT)
      (libsource (lib Deffekt-rescue) (part SWITCH-3PDT-SparkFun-Electromechanical-Deffekt-rescue) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C539AEE))
    (comp (ref SW1)
      (value SW_DPDT_x2)
      (footprint Buttons_Switches_THT:SW_CuK_JS202011CQN_DPDT_Straight)
      (libsource (lib Switch) (part SW_DPDT_x2) (description "Switch, dual pole double throw, separate symbols"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C53C33E)))
  (libparts
    (libpart (lib Connector) (part AudioJack2_Ground)
      (description "Audio Jack, 2 Poles (Mono / TS), Grounded Sleeve")
      (docs ~)
      (footprints
        (fp Jack*))
      (fields
        (field (name Reference) J)
        (field (name Value) AudioJack2_Ground))
      (pins
        (pin (num G) (name ~) (type passive))
        (pin (num S) (name ~) (type passive))
        (pin (num T) (name ~) (type passive))))
    (libpart (lib Connector) (part AudioJack3_Ground)
      (description "Audio Jack, 3 Poles (Stereo / TRS), Grounded Sleeve")
      (docs ~)
      (footprints
        (fp Jack*))
      (fields
        (field (name Reference) J)
        (field (name Value) AudioJack3_Ground))
      (pins
        (pin (num G) (name ~) (type passive))
        (pin (num R) (name ~) (type passive))
        (pin (num S) (name ~) (type passive))
        (pin (num T) (name ~) (type passive))))
    (libpart (lib Connector) (part Barrel_Jack_Switch)
      (description "DC Barrel Jack with an internal switch")
      (docs ~)
      (footprints
        (fp BarrelJack*))
      (fields
        (field (name Reference) J)
        (field (name Value) Barrel_Jack_Switch))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib Deffekt-rescue) (part SWITCH-3PDT-SparkFun-Electromechanical-Deffekt-rescue)
      (footprints
        (fp *3PDT*))
      (fields
        (field (name Reference) S)
        (field (name Value) SWITCH-3PDT-SparkFun-Electromechanical-Deffekt-rescue)
        (field (name Footprint) STOMP-SWITCH-3PDT))
      (pins
        (pin (num 1) (name O) (type passive))
        (pin (num 2) (name P) (type passive))
        (pin (num 3) (name S) (type passive))
        (pin (num 4) (name O) (type passive))
        (pin (num 5) (name P) (type passive))
        (pin (num 6) (name S) (type passive))
        (pin (num 7) (name O) (type passive))
        (pin (num 8) (name P) (type passive))
        (pin (num 9) (name S) (type passive))))
    (libpart (lib Device) (part Battery_Cell)
      (description "Single-cell battery")
      (docs ~)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarized capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D)
      (description Diode)
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_POT)
      (description Potentiometer)
      (docs ~)
      (footprints
        (fp Potentiometer*))
      (fields
        (field (name Reference) RV)
        (field (name Value) R_POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib Switch) (part SW_DPDT_x2)
      (description "Switch, dual pole double throw, separate symbols")
      (footprints
        (fp SW*DPDT*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DPDT_x2))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))
        (pin (num 3) (name C) (type passive))
        (pin (num 4) (name A) (type passive))
        (pin (num 5) (name B) (type passive))
        (pin (num 6) (name C) (type passive))))
    (libpart (lib Transistor_BJT) (part BC547)
      (aliases
        (alias BC546)
        (alias BC548)
        (alias BC549)
        (alias BC550)
        (alias BC337)
        (alias BC338))
      (description "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92")
      (docs http://www.fairchildsemi.com/ds/BC/BC547.pdf)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BC547)
        (field (name Footprint) Package_TO_SOT_THT:TO-92_Inline))
      (pins
        (pin (num 1) (name C) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name E) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Deffekt-rescue)
      (uri /home/eri/projects/git-repos/Deffekt/Deffekt-rescue.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Switch)
      (uri /usr/share/kicad/library/Switch.lib))
    (library (logical Transistor_BJT)
      (uri /usr/share/kicad/library/Transistor_BJT.lib)))
  (nets
    (net (code 1) (name "Net-(D6-Pad2)")
      (node (ref R28) (pin 2))
      (node (ref D6) (pin 2)))
    (net (code 2) (name "Net-(D6-Pad1)")
      (node (ref S1) (pin 4))
      (node (ref D6) (pin 1)))
    (net (code 3) (name "Net-(S1-Pad3)")
      (node (ref S1) (pin 9))
      (node (ref S1) (pin 3)))
    (net (code 4) (name "Net-(R2-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref S1) (pin 1)))
    (net (code 5) (name "Net-(C2-Pad2)")
      (node (ref C2) (pin 2))
      (node (ref R26) (pin 1)))
    (net (code 7) (name "Net-(C9b1-Pad2)")
      (node (ref C9b1) (pin 2))
      (node (ref SW1) (pin 3)))
    (net (code 8) (name "Net-(C8a1-Pad2)")
      (node (ref SW1) (pin 4))
      (node (ref C8a1) (pin 2)))
    (net (code 9) (name "Net-(Q2-Pad3)")
      (node (ref R10) (pin 1))
      (node (ref Q2) (pin 3)))
    (net (code 10) (name "Net-(C2-Pad1)")
      (node (ref Q1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref R6) (pin 2)))
    (net (code 11) (name "Net-(Q1-Pad3)")
      (node (ref R4) (pin 1))
      (node (ref Q1) (pin 3)))
    (net (code 12) (name "Net-(C3-Pad1)")
      (node (ref R3) (pin 1))
      (node (ref R7) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref C3) (pin 1)))
    (net (code 13) (name "Net-(C9a1-Pad1)")
      (node (ref C9b1) (pin 1))
      (node (ref R5) (pin 2))
      (node (ref C9a1) (pin 1))
      (node (ref R25) (pin 1)))
    (net (code 14) (name Earth)
      (node (ref J2) (pin S))
      (node (ref J2) (pin G))
      (node (ref J1) (pin S))
      (node (ref J1) (pin G))
      (node (ref R26) (pin 3))
      (node (ref R5) (pin 1))
      (node (ref C8b1) (pin 1))
      (node (ref R3) (pin 2))
      (node (ref C8a1) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref R22) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref R23) (pin 2))
      (node (ref S1) (pin 6))
      (node (ref S1) (pin 5)))
    (net (code 15) (name "Net-(C8b1-Pad2)")
      (node (ref SW1) (pin 6))
      (node (ref C8b1) (pin 2)))
    (net (code 16) (name "Net-(R25-Pad3)")
      (node (ref SW1) (pin 5))
      (node (ref R25) (pin 3))
      (node (ref R8) (pin 2)))
    (net (code 17) (name "Net-(C9a1-Pad2)")
      (node (ref C9a1) (pin 2))
      (node (ref SW1) (pin 1)))
    (net (code 18) (name "Net-(J1-PadT)")
      (node (ref S1) (pin 2))
      (node (ref J1) (pin T)))
    (net (code 19) (name "Net-(C14-Pad2)")
      (node (ref J1) (pin R))
      (node (ref C14) (pin 2))
      (node (ref D5) (pin 2))
      (node (ref J3) (pin 2)))
    (net (code 20) (name "Net-(J2-PadT)")
      (node (ref J2) (pin T))
      (node (ref S1) (pin 8)))
    (net (code 21) (name "Net-(R26-Pad2)")
      (node (ref S1) (pin 7))
      (node (ref R26) (pin 2)))
    (net (code 22) (name "Net-(BT1-Pad2)")
      (node (ref BT1) (pin 2))
      (node (ref J3) (pin 3)))
    (net (code 23) (name "Net-(BT1-Pad1)")
      (node (ref BT1) (pin 1))
      (node (ref R27) (pin 2))
      (node (ref J3) (pin 1)))
    (net (code 24) (name "Net-(C7-Pad1)")
      (node (ref D1) (pin 1))
      (node (ref D2) (pin 2))
      (node (ref C7) (pin 1)))
    (net (code 25) (name "Net-(C11-Pad1)")
      (node (ref Q2) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref SW1) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref D2) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref C11) (pin 1))
      (node (ref R15) (pin 1)))
    (net (code 26) (name "Net-(C11-Pad2)")
      (node (ref C7) (pin 2))
      (node (ref R16) (pin 1))
      (node (ref C11) (pin 2))
      (node (ref Q2) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref R12) (pin 1)))
    (net (code 27) (name "Net-(C12-Pad1)")
      (node (ref Q3) (pin 1))
      (node (ref C13) (pin 2))
      (node (ref C12) (pin 1))
      (node (ref R18) (pin 2))
      (node (ref D4) (pin 1))
      (node (ref D3) (pin 2))
      (node (ref R17) (pin 1)))
    (net (code 28) (name "Net-(C13-Pad1)")
      (node (ref R12) (pin 2))
      (node (ref C13) (pin 1)))
    (net (code 29) (name "Net-(C3-Pad2)")
      (node (ref C3) (pin 2))
      (node (ref R25) (pin 2)))
    (net (code 30) (name "Net-(C4-Pad1)")
      (node (ref R24) (pin 1))
      (node (ref C4) (pin 1)))
    (net (code 31) (name "Net-(C1-Pad2)")
      (node (ref C1) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 32) (name "Net-(C1-Pad1)")
      (node (ref C10) (pin 2))
      (node (ref C1) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref R9) (pin 2))
      (node (ref Q4) (pin 2)))
    (net (code 33) (name "Net-(C10-Pad1)")
      (node (ref C10) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref R9) (pin 1))
      (node (ref R13) (pin 2))
      (node (ref Q4) (pin 1)))
    (net (code 34) (name "Net-(Q3-Pad3)")
      (node (ref Q3) (pin 3))
      (node (ref R21) (pin 1)))
    (net (code 35) (name "Net-(Q4-Pad3)")
      (node (ref Q4) (pin 3))
      (node (ref R22) (pin 1)))
    (net (code 36) (name "Net-(C6-Pad1)")
      (node (ref D4) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref D3) (pin 1)))
    (net (code 37) (name "Net-(C12-Pad2)")
      (node (ref R17) (pin 2))
      (node (ref R19) (pin 1))
      (node (ref C12) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref R20) (pin 1))
      (node (ref Q3) (pin 2)))
    (net (code 38) (name "Net-(C5-Pad2)")
      (node (ref R24) (pin 2))
      (node (ref C5) (pin 2)))
    (net (code 39) (name "Net-(C5-Pad1)")
      (node (ref C5) (pin 1))
      (node (ref R19) (pin 2)))
    (net (code 40) (name "Net-(R23-Pad1)")
      (node (ref R24) (pin 3))
      (node (ref R23) (pin 1)))
    (net (code 41) (name +9V)
      (node (ref R27) (pin 1))
      (node (ref R28) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref D5) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref R13) (pin 1)))))