[[Kategorie:Hardware]]
{| border="1"
! part no.
! IC
! function
! datasheet
|+
| IC201
| MC145157P2 QQFF9208
| Serial-Input PLL Frequency Synthesizer
| http://www.datasheetcatalog.org/datasheet/motorola/MC145152P2.pdf
|+
| IC202
| MC145157P2 QQFF9208
| Serial-Input PLL Frequency Synthesizer
| http://www.datasheetcatalog.org/datasheet/motorola/MC145152P2.pdf
|+
| IC203
| KA2245 209
| FM IF System for Car Radios
| http://www.datasheetcatalog.org/datasheet/SamsungElectronic/mXvvqzt.pdf
|+
| IC204
| KA2245 209
| FM IF System for Car Radios
| http://www.datasheetcatalog.org/datasheet/SamsungElectronic/mXvvqzt.pdf
|+
| IC205
| MC4558C 208C
| High Frequency Amplifiers and Comparators
| http://www.datasheetcatalog.org/datasheet/motorola/MC34181.pdf
|+
| IC206
| MC4558C 208C
| High Frequency Amplifiers and Comparators
| http://www.datasheetcatalog.org/datasheet/motorola/MC34181.pdf
|+
| IC207
| MC14053BCP FFMG9205
| Analog Multiplexer / Demultiplexer
| http://www.datasheetcatalog.org/datasheet/motorola/MC14053BCP.pdf
|+
| IC208
| C1406HA 9124NE247
| Dual Attenuator
| http://www.datasheetcatalog.org/datasheets/400/502589_DS.pdf
|+
| IC209
| MC14053BCP FFPB9206
| Analog Multiplexer / Demultiplexer
| http://www.datasheetcatalog.org/datasheet/motorola/MC14053BCP.pdf
|+
| IC301
| MC7805C 208
| THREE TERMINAL POSITIVE FIXED VOLTAGE REGULATOR
| http://www.datasheetcatalog.org/datasheet/motorola/MC7809.pdf
|+
| IC302
| MC7805C 208
| THREE TERMINAL POSITIVE FIXED VOLTAGE REGULATOR
| http://www.datasheetcatalog.org/datasheet/motorola/MC7809.pdf
|+
| IC303
| LM317T 204
| 1.2V TO 37V ADJUSTABLE VOLTAGE REGULATOR
| http://www.datasheetcatalog.org/datasheet2/1/03cgthpfat4t4ly5kfp5lpwladfy.pdf
|+
| IC304
| MC7905C 153
| 1A, 5V, Negative Voltage Regulator
| http://www.datasheetarchive.com/pdf-datasheets/Databooks-2/Book510-3136.pdf
|+
| IC305
| MC7812AC 202
| THREE TERMINAL POSITIVE FIXED VOLTAGE REGULATORS
| http://www.datasheetcatalog.org/datasheet/motorola/MC7809.pdf
|+
| IC306
| MC7805C 208
| THREE TERMINAL POSITIVE FIXED VOLTAGE REGULATOR
| http://www.datasheetcatalog.org/datasheet/motorola/MC7809.pdf
|+
| IC401
| LM324 141B
| LOW POWER QUAD OPERATIONAL AMPLIFIER
| http://www.datasheetcatalog.org/datasheet/stmicroelectronics/2156.pdf
|+
| IC501
| LSC404163P 63JH8LLZV9204
| ? discontinued ?
| http://chip-sale.com/catalog8/cat/4959.html
|+
| IC502
| CAT35C104P C99207B
| 4K-Bit SERIAL E2PROM
| http://www.alldatasheet.com/datasheet-pdf/pdf/123188/CATALYST/CAT35C104.html
|+
| IC503
| MC145157P2 QQFF9208
| Serial-Input PLL Frequency Synthesizer
| http://www.datasheetcatalog.org/datasheet/motorola/MC145152P2.pdf
|+
| IC801
| CAT35C104P C99207B
| 4K-Bit SERIAL E2PROM
| http://www.alldatasheet.com/datasheet-pdf/pdf/123188/CATALYST/CAT35C104.html
|+
| Q109
| D882-Y 207
| NPN(for the output stage of 3 watts audio amplifier, voltage regulator, DC-DC converter and relay driver)
| http://www.datasheetcatalog.org/datasheet/nec/2SD882.pdf
|+
| Q305
| B834 Y-207
| POWER TRANSISTORS(3.0A,60V,30W)
| http://www.datasheetcatalog.org/datasheet/mospec/2SB834.pdf
|}
[[image:Multistar 2000 satellite receiver 1.JPG|300px|]][[image:Multistar 2000 satellite receiver 2.JPG|300px|]]
[[image:Multistar 2000 satellite receiver 3.JPG|300px|]][[image:Multistar 2000 satellite receiver 4.JPG|300px|]]
[[image:Multistar 2000 satellite receiver 5.JPG|300px|]][[image:Multistar 2000 satellite receiver 6.JPG|300px|]]
[[image:Multistar 2000 satellite receiver 7.JPG|300px|]][[image:Multistar 2000 satellite receiver 8.JPG|300px|]]
[[image:Multistar 2000 satellite receiver 9.JPG|300px|]][[image:Multistar 2000 satellite receiver 10.JPG|300px|]]
[[image:Multistar 2000 satellite receiver 11.JPG|300px|]][[image:Multistar 2000 satellite receiver 12.JPG|300px|]]
[[image:Multistar 2000 satellite receiver 13.JPG|300px|]]
